Class: 	FIFTEEN-MINUTE TESTĐỀ 1

Name:		
1. [image: ]  is the logo of ___________.
	A. Audi TT	B. Renault	C. Porsche	D. Smart
2. [image: ] is the logo of ___________.
	A. Lamborghini		B. Porsche	C. Jaguar	D. Ferrari
3. The __________ is a round hole bored in the block. It guides piston movement.
	A. cylinder		B. cylinder head	C. camshaft	D. crankshaft
4. The __________ controls the opening of the valves.
.	A. camshaft		B. crankshaft  	C. rocker arm 	D. lifter
5. Compression makes the explosion more __________.
.	A. weaker                   	B. stronger                  	C. powerful                          D. All are correct
6. The compression ratio in petrol engine is kept less than in Diesel engine because __________.
	A. higher or equivalent compression ratio in petrol engines is not possible due to pre-ignition
	B. it is just customary to have less compression ratio in petrol engines
	C. less compression ratio gives better performance
	D. it makes petrol engines lighter
7. A ______ is a part of the roof of a car that you can open to let air and light in.
	A. headlight		B. sunroof	C. door	D. sill
8. The ________ provides the energy to propel the vehicle and operate the other systems.
	A. frame		B. chassis	C. engine	D. body
9. The connecting rods are generally made of __________ shaped cross-section.
	A. I		B. H 	C. C	D. L

10. If your seat is too low, you will adjust the ________.
	A. seat belt	B. seat position	C. headrest 	D. seat height
11. A/ an __________ is a metal or plastic disc fitted to the centre of a road wheel.
	A. badge	B. wheel trim	C. exhaust pipe	D. door 
12. The __________ is a small cavity (hollow area) between the top of the piston and the bottom of the cylinder head 
.	A. block                     B. connecting rod    	C. combustion chamber  	D. crankcase
13. The motion of the cam is transferred to the valves through __________.
A. pistons	B. camshaft pulley	C. rocker arms	D. valve stems
14. ________ provides a combustible air-fuel mixture to power the engine.
	 A. Electrical system	B. Exhaust system	C. Emission control system	D. Fuel system
15. The front bumper absorbs small __________ in accident.
.	A. effects                  B. knocks               	C. pings                           	D. impacts
16. The first automobile was powered by ________ engine.
	A. internal combustion engine	B. diesel 		C. steam	D. gasoline 
17. The function of an alternator in an automobile is to ________.
	A. continually recharge the battery	C. supply electric power
	B. convert mechanical energy into electrical energy    D. partly convert engine power into electric power
18. If the engine coolant leaks into the engine oil, then engine oil ________.
	A. turns black	B. appears milky	C. becomes foamy                D. none of these
19. The battery is an electrochemical device, which means battery ________.
		A. has curved plates instead of flat plates	C. uses chemical action to provide electricity
	B. makes chemicals by mechanical means	D. does not use an electrolyte
20. A ________ is an instrument used to indicate the level of fuel contained in a tank.
    	A. fuel gauge 		 B. coolant temperature gauge 
	C. fuel consumption		 D. engine oil temperature gauge
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