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Description

B 4935403

WHAT CAN WE DO TO HELP
fyou would like information about pricing and delivery, Our
sales will contact you shortly.
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Danh myc cira hang [ Motor Mode! SZGH-04010D

~ CNC Controller Rated Power(W) 100

Lathe Rated Voltage(V) 20

Milling Rated Current(A) 2o
Router

Servo Motor Rated Specd(RPM) 3000

Servo Driver Rated Torque(NM) 03

~ Step Motor Peak Torque(NM) 0.64

Stepper motor Voltage Constant(v/ o0y 3238

Closed Loop Stepper
Motor

Torque Coeflicient(NM/A) 053

~ Step Driver Rotor Inertia(Kg m?) 00514104

Stepper Driver Line-Line Resistance(Q2) 34

Closed Loop Stepper
Driver

Line-Line Inductance(mH) 40

Spindle Servo Motor Machanical Time-Constanttts) Lig

Spindle Servo Driver Encoder Resolution(PPR) 2500

CNC Spare Parts Insulation Class ClassB
Others.

Safety Class P65
‘The Operating of Temperature:-20'C~+40°C

ban chay Evironmental Condition Humidity Below 90%RH(No dewing)

Weight(KG) 047
st

San pham Hinh Anh





