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Presentation Lexium Linear Motion
Lexium TAS linear tables

Lexium TAS linear tables support high-precision linear positioning of heavy loads at
high feed forces.

This level of performance is made possible by the drive system, which uses a
preloaded ballscrew.

The linear tables' design is based on an aluminium profile capable of supporting
substantial pressure without bending. They are able to move loads of up to 150 kg,
depending on the model

To facilitate integration into a large number of applications, there are a range of
different configuration options. These include table length, different pitches for the
ballscrew, different mounting options for the drive element, etc. (see page 18).

Lexium TAS 4eS linear table with mofor and gearbox mounted  Schneider Electric offers a number of drive elements which can be used to drive
Lexium TAS linear tables (2) (see page 19).
Third-party drive elements can also be used under certain conditions. Contact our
Customer Care Centre for further details
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