 Bộ nguồn xung S8JC-150 12-P
Bộ nguồn xung S8JC150 24-P
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Cảm biến chuyển động   
CẢM BIẾN HỒNG NGOẠI TẦM XA KM-P314 ( thay cho PA-465 PIR)
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Cảm biến quang thu phát chung
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Cảm biến từ  TL 05MC1
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Cảm biến nhiệt
LM 35
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Cảm biến đo nhiệt
CẢM BIẾN NHIỆT (đầu dò nhiệt) E52MY-PT10C
Platinum-resistance thermometer
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Máy đo nhiệt K3MA-L-C 100-240VAC
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Cảm biến đo tần số K3MA-F – A2
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Cảm biến đa năng Timer/counter Autonics	CT6M-2P
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PLC Mitsubitshi FX1N
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cảm biến khói  FDK246
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Bộ điều khiển trung tâm báo cháy GST 104 A
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K3MA-LC 100-240VAC
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K3MA-FA2  100-240VAC
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Autonics 5P4M
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DOMINO  gắn trên mạch in
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Động cơ Bước     
Động cơ Servo         
Driver động cơ Bước
Driver động cơ Servo 
Mạch điều khiển CNC - USB controler
Mạch in mạch điều khiển động cơ
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= DiN-size of 45 x 86 mm (H x W)

= Highly visible, negative transmissive backit LCD display.

= 3 models: K3MA-J (Process), K3WA-L (Tempsrature)
and KIMA- (Frequency)

* 14.2-mmwhigh characters; S igits (-18998 to 99898)

« Front-panel P66




image10.jpeg




image11.jpeg
PL%AIGON

\/ -




image12.png
) fdk_246.pdf (SECURED) - Foxit Reader - [fdk_246.pdf (SECURED)]
[ File Edt View Comments Forms Took Help

FEATURES

(1) Small monitoring current of 45 u A

(2) 2-wire system

(3) Alarm response lamp (LED)

(4) Simple mounting

(5) Very easy maintenance

(6) Very low profile

(7) Conventional type

(8) Approved by Japan Fire Equipment Inspection Institute

DESCRIPTION

The FDK series photoelectric smoke detectors detect
combustion products (smoke) generated by a fire, and
transmit an alarm signal to the fire alarm control panel.
The photoelectric smoke detector can deteot a fire in an
earlier stage than a heat detector. Generally, this
detector is installed in the spaces such as basements,
ordinary fioors, corridors, staircases, elevator shafts.

OPERATING PRINCIPLE AND FUNCTION WITH RECESS MOUNTING BASE
The photoelectric smoke detector is composed of a light
source, light sensing element, light shielding element
and detecting chamber. The light source (a
light-emitting diode) emits light at intervals of about 3.5
seconds, which does not reach the light sensing
element (photo diode) under normal conditions because
of the light shielding mold. If smoke enters the detecting
cchamber, the light from the light source is scattered by
smoke particles and reaches the light sensing element
The light reaching the light sensing element varies with
'smoke density and if it exceeds the predetermined level,

s1/2 Size: [8.27 % 11.69 in]
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