UNIT 5
Advantages of the CNC Machines

I. READING COMPREHENSION
Advantages of the CNC Machines
Advantages of the CNC Machines 
There are various valid reasons for the popularity of the CNC machines over the NC machines, let us see some of them.
1) Part program tape and tape reader: In the older CNC machines the part program tape and the tape reader is still required, but they are used only for feeding the program into the memory of the computer. Once the program is saved into the memory, the tape is no more required and the program stored in the memory can be used repeatedly. Thus the tape and the tape reader that poses the major maintenance problems are done away with. In fact the latest CNC machine don’t even require the tape and tape reader, for the program of instructions are fed directly into the mini or microcomputer via the control panel of the computer.
2) Editing the program: Since the program of instructions is saved in the computer memory, they can be edited and changed as per the requirements. Thus the CNC system is highly flexible. One can also make necessary changes in the program for providing variable speeds and feeds for the manufacture of the jobs resulting in economic manufacturing. Even the NC tape used for the programming in CNC machines can be corrected and optimized since it allows changes in the tool path, speed, feed etc.

3) Metric conversion: The CNC machine allows the conversion of tapes prepared in the metric system into the SI system of measurements. Thus programmer does not have to re-enter the whole program of instructions merely because of the different units of measurements used in the program.
4) Highly flexible: The CNC machines are highly flexible. One can easily make the changes in the program and store them as the new program. One can also introduce new control options like the new interpolation scheme quite easily. It is easier to make updates in the CNC machines with lesser cost; hence risk of the obsolescence of the CNC machine is reduced.
5) Easier programming: The programs are written in the CNC machine using language which has statements similar to the ordinary English language statements. The programmer can easily master the CNC programming language and use it for the wide range of the machining operations of the job. The programmer can set the various dimension of the job, the machining operations to be carried out and their sequence, the amount of metal to be removed in each cutting operation, the speed of cutting, etc. The program of instructions is written as per the available size of the raw materials and also the surface finish required for the final finished job. Some of the programs take the form of the macro subroutines stored in the memory of the CNC machine and the programmer can use them frequently whenever required. Some of the programs are stored in the library and they can be used wherever required completely or as a small part of the big program.






II. VOCABULARY
· Valid(a):	hợplý, cócơsở
· Popularity(n):	Sựphổbiến
· tape reader:	thiếtbịđọcbăng (đụclỗ)	
· required(a):	bắtbuột, cầnthiết	
· Once(adv):	chỉmộtlần, trướckia
· Store(v):	tíchtrữ, cấttrongkho
· repeatedly:	lậplại
· thus(adv):	theocáchđó, nhưvậy
· pose(v):	đềraluậnđiểm
· maintenance(n):	sựbảodưỡng (máymóc)
· be done away with:	
· latest(a):	gầndâynhất
(late– later – latest)	
· control panel:	bảngđiềukhiển
· 	system control panel	bảngđiềukhiểnhệthống
· Edit(v):	(tin học) soạnthảo, hiệuđính
· Necessary(a):	cầnthiết, quantrọng
· Variable(a):	cóthểthayđổiđược
· Resulting(a):	do, nguyênnhân
· Optimize(v):làmchocànghoảnchỉnhcàngtốt, tốiưuhóa
· tool path:	đườngchạydao, đườngdẫncôngcụ
· Metric(n):	tiêuchuẩnđolường
· conversion:	sựchuyểnbiến
· measurement:	hệthốngđolường
· to re-enter:	lạitrởvào
· merely(adv):	chỉ (only)
· unit(n):	đơnvị
	
·  option(n):	(tin học) tùychọn
· Interpolation(n):	(toánhọc) phépnộisuy
· Scheme(n):	sựsắpxếptheohệthống
· Update(v):	làmchocậpnhật, hiệnđạihóa
· Lesser(a):	nhỏhơn, kémhơn (cấp so sánhcủa little)	
· risk(n):	sựrủiro
· obsolescence(n):	sựlỗithời, khôngcòndùngnữa
· similar to:	giốngnhư
· master:	nắmvững, điềukhiển
· a widerange of:	đủloại
(awiderange of prices : đủloạigiácả)
· amount of:	sốlượnglớncủacáigì
· to be removed:	đượcdờiđi, bịchuyểnchỗ	
· surface (n):	bềmặt
· form:	hìnhdạng
· macro(a):	phạm vi rộng
· subroutine:	(vi tính) thủtục con
· economic manufacturing:      chiếnlượckinhtếtrongsảnxuất
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Task 1. Answer the following questions
1. How many Advantages are there in the CNC Machines?
…………………………………………………………………………………
…………………………………………………………………………………
2. Which ones?
…………………………………………………………………………………
…………………………………………………………………………………
3. In the latest CNC machines  is the part program tape and the tape reader  required? Why (not)?
…………………………………………………………………………………
…………………………………………………………………………………
4. What is the NC tape used for ? Can it be corrected in the CNC machines?
…………………………………………………………………………………
…………………………………………………………………………………
5. Why is the CNC system  highly flexible?
…………………………………………………………………………………
…………………………………………………………………………………




Task 2. Are these sentences true or false? Correct the false sentences.
1. The CNC machine doesn’t allow the conversion of tapes prepared in the metric system into the SI system of measurements.
…………………………………………………………………………………
….………………………………………………………………………………
2. The CNC machines are a little flexible. .
…………………………………………………………………………………
….………………………………………………………………………………
3. It is easier to make updates in the CNC machines with lesser cost .
…………………………………………………………………………………
….………………………………………………………………………………
4. The programs are written in the CNC machine using language which has statements similar to the ordinary English language statements.
…………………………………………………………………………………
….………………………………………………………………………………
5. The programmer can easily master the CNC programming language.

--------------------------------------------------------------------------------------






Task 3. Choose the best answer
1. There are various valid reasons for the popularity of the CNC machines -----
 the NC machines .
A. In 	B. under	C. over	D. of
2. The part program tape and the tape reader are used only for -------the program into the memory of the computer.
A. eating	B. feeding	C. buying	D. mading
3. Once the program is saved into the memory, the tape is  more required.
A. no	B. any	C. many	D. much
4. the program of ………. is saved in the computer memory, they can be edited and changed as per the requirements..
A. measurements   B. reasons	C. coins	D. instructions
5. The CNC system can also make ------- changes in the program .
A. unnecessary	B. necessary        C. uncertain        D. patient


