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1. After being pumped through a diverter or priority valve, water circulates around either one of two loops of pipework, which acts as ______________________.


A. radiator 

B. heat exchanger
C. condenser
D. compressor
2. Newer refrigerants which are less harmful to the environment, such as ____________________, 
are gradually replacing R12.


A. KLEA 134a

B. KLEF 134b
C. KLAE 134a
D. KLAF 134b

3. The ________________ built into the control unit keeps the memory of the control unit informed.


 

A. electronic drum        
B. electronic thermometer




C. electronic memory     
D. electronic clock

4.  _____________________ is the transfer of heat by waves similar to light waves or radio waves. 


A. Radiator

B. Conduction
C. Conductor
D. Radiation

5. The temperature at which liquid changes into vapor is called as “____________________”.



A. melting point

B. boiling point
C. expansion point
D. none of them 

6. Electrical engineering is not about ______________________.



A. the generation of electricity
B. the distribution of electricity 



C. the installation of electricity
D. communications

7. Solids can be _____________________ easily by means of transport.


A. carried

B. circulated
C. piped
D. pumped

8. ___________________ is a device in the fridge that regulates temperature so that the food is not 
over-frozen.


A. Thermostat

B. Button
C. Compressor
D. Cylinder

9. The house ______________________ by Mary.

A. clean 

B. cleans
C. is cleaning
D. was cleaned

10. _____________________ is the flow of heat by means of a fluid medium, either gas or liquid, normally air or water.                 


A. Convector             B. Conduction
C. Conductor              
D. Convection

11. The flow of gas to the burner is ____________________ by a valve which can be operated by 
a time switch or by a boiler thermostat, hot water cylinder thermostat, or by a thermostat located 
in one of the rooms.


A. controlled

B. controls
C. control
D. controlling 
12. ___________________ is a piece of electrical equipment in which food is kept cold so that 
it stays fresh.

       A. Washing machine
  B. Central heating          C. Refrigerator          D. Air - conditioner
13. The control system of a modern washing machine has to take into account several different factors such as door position, water level, water temperature, wash and spin times and _______________________.


A. large of drum 
B. size of drum
C. shape of drum
D. speed of drum

14. The first and most important of these laws is the fact that energy can neither be ______________ nor ___________________, but can be converted from one type to another. 




A. create, destroy

B. destroy, create           



C. created, destroyed            
D. created, destroying
15. The form of energy that produces feeling of hotness is called as “______________________”.


A. work

B. heat
C. energy
D. none 

16. ___________________: cars, trains, ships and planes are all products of mechanical engineering.


A. Transports

B. Transport
C. Transportation
D. to Transport

17. _____________________ the hot water flows through the radiators, the hot water loses heat.


A. As

B. When
C. After
D. Until

18. If a gas expands, it _________________________. 

A. cool down

B. cools down
C. cool up
D. cools up 

19. The rising water level is checked by __________________________.






A. the water valve
 
B. the water thermostat
  





C. the water level sensor

D. the water level      

20. ____________________________ is a very good heat conductor.


A. Wood

B. Plastic
C. Metal
D. Mental

21. The ________________________ is made of tubes of cast iron or copper, which resist corrosion.


A. heat exchanger

B. diverter valve
C. thermostat
D. flue
22. One common refrigerant is a compound of _______________________.


A. carbon

B. chlorine
C. All are wrong.
D. All are correct.
23. The seals _______________________ at the zoo twice a day.

A. is feed

B. are fed
C. is fed
D. are feed

24. The ____________________ of heat travel is in direct proportion to the temperature difference between the two bodies.


A. scale

B. size

C. rate
 
D. weight
25. Which of the following is not the process of transfer of heat ? _____________________.

A. Radian        

B. Convection
C. Radiation
D. Conduction
26. Electrical engineering is concerned with the production and distribution of electricity to home, offices … and installation and maintenance of the equipment ________________ in these processes.


A. involve

B. involved
C. involves
D. involving

27. The first stage in operating sequence of gas central heating is that ________________________.





A. water is circulated through a heat exchanger
   




B. water is heated by gas burners






C. cold water from the radiators returns to the boiler
   




D. the loop returns to the boiler for re-heating
28. If a wire cuts a magnetic field, a current is _______________________ in the wire.

A. resisted

B. generated
C. radiated
D. induced
29. ________________________ rotates the drum in washing machine.


A. Heater

B. Motor
C. Fan
D. Solenoid valves

30. Temperature is ______________________.


A. a form of heat transfer where energy is radiated in the form of rays



B. a form of heat transfer




C. a form of energy contained in an object associated with the motion of molecules

D. a measure of the hotness or coldness of an object
31. _____________________ is concerned with developing components and equipment for communication, computing and so on.




A. Electronic engineering
B. Civil engineering   




C. Electrical engineering    
D. Mechanical engineering
32. The _____________________ is a tube used to convey water, gas, oil, or other fluid substances.


A. pump

B. valve
C. thermostat
D. pipe

33. ________________________ is a device that cools gas in order to change it into liquid.


A. Compressor

B. Condenser
C. Capillary tube
D. Evaporator

34. In the washing machine, _________________________ senses when the drum is full of water and reports it to the control unit.


A. temperature sensor 
        B. fan               

C. pressure sensor              D. solenoid valve

35. Heat transfer in liquid and gases takes place by ________________________.


A. conduction
  B. convection 
 C. radiation  
 D. conduction and convection
36. __________________ engineering deals with the design and manufacture of tools and machines.



A. Mechanical

B. Civil
C. Electrical
D. Electronic 
37. The pilot light, the flue, the finned heat exchanger and the pump are the components of __________________.


A. washing machine

B. refrigerator 
C. central heating
D. sewing machine

38. _______________________ is the flow of electricity.


A. Force

B. Wire
C. Current
D. Spring

39. In the washing machine, ______________________ controls the flow of water into the machine.


A. heater

B. temperature sensor
C. motor
D. solenoid valves

40. Water freezes at _______________________ 0F and O0C


A. 30

B. 31
C. 32
D. 33

41. If a pressure is applied to the surface of an enclosed fluid, it is transmitted equally throughout 
the ___________________.                   

A. radiator

B. condenser

C. heat

D. fluid 
42. ______________________ is a long tube in the shape of a zigzag in structure of fridge.


A. Condenser

B. Evaporator
C. Compressor
D. Capillary tube

43. The temperature ______________________ measures the water temperature and signals it 
to the control unit.





A. level

B. sensor        
C. scale
D. Ø
44. _____________________ is the flow of heat through a substance. Actual physical contact is required for heat transfer to take place between two bodies by this means.


A. Convector

B. Conduction
C. Conductor
D. Convection

45. The process of transfer of heat in liquids & gases is called as “____________________”.


A. conduction

B. radiation
C. convection
D. absorption


46. Most gas central heating works on at the “__________________________” system of heat transfer between water flowing through pipes.
   

A. cold


B. cool
  

C. wet      
D. hot
47. The compressor compresses the gas so that it __________________________.


A. cools down

B. cools up
C. heats down
D. heats up

48. Adjusting the sound of a TV is an example for the control may change the _________________.






A. size of the input         

B. shape of the input             





C. size of the output        

D. shape of the output

49. _______________________ is that branch of science dealing with the mechanical action of heat. 


A. Thermodynamic

B. Thermoduric
C. Thermo cycle
D. Thermostatic
50. If a force is applied to a ___________________________ fixed at one end, it extends in proportion to the force.


A. radiator

B. loop
C. spring
D. condense
The End of the Test
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