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1. A ________________ is any physical substance which keeps its shape even when not contained.


A. solid

B. vapor
C. water
D. fluid

2. The refrigeration process begins in the __________________.


A. condenser

B. evaporator
C. compressor
D. capillary tube

3. The temperature sensor is a type of ____________________which fits inside the washer drum.


A. clock

B. thermostat
C. thermometer
D. unit control

4. The sun's energy is transferred to the Earth by ___________________.


A. radiator

B. convention
C. convector
D. radiation

5. It is the process of heat transfer from a hot body to a colder body without heating the space between the two is called as: “__________________”.


A. Conduction

B. Radiation
C. Convection
D. Absorption

6. Mining and medical engineering ____________ partly _____________ mechanical and electrical.


A. belongs/to

B. belongs/of
C. belong/to
D. belong/of

7. ________________ the water temperature reaches the right level, the gas control valve shuts off.


A. As

B. When
C. After
D. Until

8. _________________ is not the component of the washing machine.


A. Condenser

B. Door lock
C. Control unit
D. Shock absorber

9. When a wash program first start, it has to ____________ which allow the water ________________.


A. close the valves/in
B. open the valves/in 


C. close the valves/out
D. open the valves/out

10. Air may be heated by a furnace, and then discharged into a room to heat objects in the room by ______________. 


A. convector

B. radiation
C. radiator
D. convection

11. Water is circulated through a heat exchanger ________________ the burner.


A. on

B. in
C. above
D. at

12. Refrigeration is based on __________________ principles.


A. 1

B. 2
C. 3
D. 4

13. Most washing machines use 53 rpm for _________________.


A. spinning

B. the load 
C. washing 
D. mixing

14. The second important law of thermodynamics is that _______________ always travels from a warm object to a colder one.


A. heat

B. lubricant
C. refrigerant
D. coolant
15. __________________ is neither created nor destroyed it can be only changed one form to another.


A. Work

B. Heat
C. Energy
D. Mass of body

16. _________________ deals with cable, switchgear and connecting up electrical equipment.


A. Electrical installation
B. Electricity generation


C. Electrical maintenance
D. Electrical services

17. The last stage in operating sequence of gas central heating is ___________________.


A. the loop returns to the boiler for re-heating

B. Water is heated by gas burners



C. Cold water from the radiators returns to the boiler
D. Water is circulated through a heat exchanger

18. If a wire cuts a magnetic field, _____________________.


A. a current is induced in the wire. 
B. it extends in proportion to the force.


C. it heats up

D. it sets up a magnetic field around the wire.

19. In the washing machine, ____________________ pumps water out of the drum.


A. motor

B. pump
C. shock absorber
D. fan

20. ________________ has so much resistance to heat flow it can be used as insulation.


A. Asbestos

B. Metal
C. Copper
D. Steel

21. ___________________ located in the boiler causes the gas control valve to shut off when the water temperature reaches the pre – set level.


A. Thermostat

B. Priority valve
C. Diverter valve
D. Pump

22. Refrigeration preserves food by _____________________its temperature.


A. lower

B. lowers
C. lowering
D. low 

23. The ____________________ is the heart of the system in the washing machine.


A. control unit

B. drum
C. motor
D. fan 

24. Heat can travel in any of three ways: _____________________.


A. radiation, conduction, or convector
B. radiation, conduction, or convection 


C. radiator, conduction, or convector
D. radiator, conductor, or convection

25. The process of transfer of heat in solids is called as “_____________________”.


A. Convection

B. Radiation
C. Conduction
D. None of them 

26. ___________________ is not the component of Gas central heating.


 A. Boiler thermostat

B. Priority valve
C. Loop of pipework
D. Heater

27. The gas condenses back into_________________________.


A. solid

B. liquid
C. vapour
D. fluid 

28. In the washing machine, ________________ absorbs the shock of the spinning drum when loaded.


A. pressure sensor

B. temperature sensor
             C. shock absorber
         D. heater

29. Which of the following is the worst conductor of heat ? ________________.

A. glass

B. plaster
C. aluminum
D. brass

30. ___________________ includes automobile, aeronautical and heating and ventilating.


A. Mechanical engineering
B. Civil engineering 


C. Electrical engineering
D. Electronic engineering

31. _______________ is a device for controlling the passage of fluid through a pipe or duct, especially an automatic device allowing movement in one direction only.


A. Pump

B. Valve
C. Thermostat
D. Pipe

32. __________________ is circulated around the fridge, where it undergoes changes in pressure and temperature and changes from a liquid to a gas and back again.


A. Refrigerant

B. Refrigeration
C. Refrigerator
D. Fridge 
33. In the washing machine, ________________ senses whether the door is open or shut and reports it to the control unit.


A. pump
  B. temperature            
 C. pressure sensor
               D. door lock and sensor

34. The relation between Fahrenheit and Centigrade scales can always be ___________________ by 
the following formulas.


A. establish

B. establishing
C. established
D. establishes
35. _______________ is about the generation and distribution of electricity and its many applications.


A. Mechanical engineering
B. Civil engineering 


C. Electrical engineering
D. Electronic engineering

36. The ___________________ is a part of a cooker, lamp, etc. that emits a flame.


A. switch

B. pump
C. boiler
D. burner

37. ___________________the warm gas passes through the condenser, it heats the surrounding and cools down.


A. As

B. When
C. After
D. Until

38. _________________ raises the temperature of the water.


A. Heater

B. Pump
C. Fan
D. Shock absorber

39. Water boils at sea level at _____________________ 0F and 1000C.


A. 210

B. 211
C. 212
D. 213
40. We can use “___________________” to show that one action is followed by another action.


A. as

B. until
C. after
D. when 

41. Liquid leaving the condenser has to flow down the very narrow tube. The very narrow tube is known as __________________.


A. condenser

B. evaporator
C. compressor
D. capillary tube
42. If the water temperature is too low, the control unit will switch on _____________________.


A. the boiler

B. the burner
C. the heater
D. the drum

43. Conduction is a highly efficient means of heat transfer as any service-man who has touched a piece of hot metal can ___________________.  


A. test

B. testify
C. testified
D. testifies

44. A cold steel spoon is dipped in a cup of hot milk. It transfers heat to its other end by the process of _______________.


A. convection

B. conduction
C. absorption
D. radiation

45. In conventional boilers, water is heated by ___________________.

A. gas 

B. gas burner
C. gas central heating
D. gas boiler

46. Refrigerant has a very ______________________ boiling point: -290C.


A. low

B. high
C. constant
D. average 

47. ____________________ cools the pump motor.


A. Heater

B. Fan
C. Pump
D. Pressure sensor 

48. There are certain fundamental principles of nature, often called laws of thermodynamics, which govern our ________________ here on Earth, several of which are basic in the study of refrigeration.


A. existence

B. exist
C. existent
D. existing

49. The capacity to do work is called as _____________________.


A. heat

B. energy
C. work
D. none 

50. Certain chemicals are added to glue to _______________________ it.


A. hard

B. harden 
C. hardly
D. hardenly
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