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1. After being pumped through a diverter or priority valve, water circulates around either one of two loops of pipework, which acts as ______________________.


A. pump 

B. loops
C. valve
D. pipe
2. Newer refrigerants which are less harmful to the environment, such as _________________,  are gradually replacing R12.


A. KLEA 134a

B. KLEF 134b
C. KLAE 134a
D. KLAF 134b

3. The __________________ built into the control unit keeps the memory of the control unit informed.


 

A. electronic drum        
B. electronic thermometer




C. electronic memory     
D. electronic clock

4.  ___________________ is the transfer of heat by waves similar to light waves or radio waves. 


A. Radiator

B. Conduction
C. Conductor
D. Radiation

5. The house ____________________ by Nga.




A. cleans

B. was cleaned
C. cleaning
D. to clean
6. Electrical engineering is not about ______________________.



A. the generation of electricity
B. the distribution of electricity 



C. the installation of electricity
D. communications

7. A new car _____________________ by Tom.


A. is being sold

B. sell
C.to sell
D. selling
8. ____________ is a device in the fridge that regulates temperature so that the food is not over-frozen.


A. Thermostat

B. Button
C. Compressor
D. Cylinder

9. The house ____________________ by Mary.

A. clean 

B. cleans
C. is cleaning
D. was cleaned
10. _____________________ is the flow of heat by means of a fluid medium, either gas or liquid, normally air or water.                 

A. Convector             B. Conduction
 C. Conductor             D. Convection

11. The flow of gas to the burner ___________________ by a valve which can be operated by a time switch or by a boiler thermostat, hot water cylinder thermostat, or by a thermostat located in one of 
the rooms.


A. is controlled

B. controls
C. control
D. controlling 

12. _______________ is a piece of electrical equipment in which food is kept cold so that it stays fresh.


 A. Washing machine
  B. Central heating
C. Refrigerator
D. Air - conditioner
13. The control system of a modern washing machine has to take into account several different factors such as door position, water level, water temperature, wash and spin times and ___________________.


A. large of drum

B. size of drum
C. shape of drum
D. drum speeds 

14. The first and most important of these laws is the fact that energy can neither be _______________ nor _________________, but can be converted from one type to another. 




A. create, destroy

B. destroy, create           



C. created, destroyed            
D. created, destroying
15. The form of energy that produces feeling of hotness is called as “______________________”.


A. work

B. heat
C. energy
D. none 

16. ___________________: Cars, trains, ships and planes are all products of mechanical engineering.


A. Transports

B. Transport
C. Transportation
D. To transport

17. _____________________ the hot water flows through the radiators, the hot water loses heat.


A. As

B. When
C. After
D. Until

18. If a gas expands, it _________________________. 

A. cool down

B. cools down
C. cool up
D. cools up 

19. The rising water level is checked by __________________________.






A. the water valve
 
B. the water thermostat
  





C. the water level sensor

D. the water level      

20. ____________________________ is a very good heat conductor.


A. Wood

B. Plastic
C. Metal
D. Mental

21. The ________________________ is made of tubes of cast iron or copper, which resist corrosion.


A. heat exchanger

B. diverter valve
C. thermostat
D. flue
22. One common refrigerant is a compound of __________________, R12, and __________________.



A. carbon
    B. chlorine
C. All are wrong.
D. All are correct.
23. The seals ______________________ at the zoo twice a day.

A. is feed

B. are fed
C. is fed
D. are feed
24. The ____________________ of heat travel is in direct proportion to the temperature difference between the two bodies.


A. scale

B. size

C. rate
 
D. weight
25. Which of the following is not the process of transfer of heat ? _____________________.

A. Radian        

B. Convection
C. Radiation
D. Conduction
26. __________________ engineers are concerned with the production and distribution of electricity 
to home, offices, and the installation and maintenance of the equipment involved in these processes.


A. Mechanical

B. Electrical
C. Electronic
D. Medical
27. The first stage in operating sequence of gas central heating is that ________________________.





A. water is circulated through a heat exchanger
   




B. water is heated by gas burners






C. cold water from the radiators returns to the boiler
   




D. the loop returns to the boiler for re-heating
28. If a wire cuts a magnetic field, a current is _______________________ in the wire.

A. resisted

B. generated
C. radiated
D. induced
29. _______________________ rotates the drum in washing machine.


A. Heater

B. Motor
C. Fan
D. Solenoid valves

30. Temperature is ______________________.


A. a form of heat transfer where energy is radiated in the form of rays



B. a form of heat transfer




C. a form of energy contained in an object associated with the motion of molecules

D. a measure of the hotness or coldness of an object

31. _____________________ engineering is concerned with developing components and equipment 
for communication, computing and so on.




A. Electronic

B. Civil 
C. Electrical   
D. Mechanical 
32. The ________________________ is a tube used to convey water, gas, oil, or other fluid substances.


A. pump
B. valve
C. thermostat
D. pipe

33. _________________________ is a device that cools gas in order to change it into liquid.


A. Compressor

B. Condenser
C. Capillary tube
D. Evaporator

34. In the washing machine, _________________________ senses when the drum is full of water 
and reports it to the control unit.


A. temperature sensor 
        B. fan               

C. pressure sensor              D. solenoid valve

35.  The food ______________________ by Loan.



A. cook


B. will be cooked
C. cooked



D. cooking

36. ___________________ engineering deals with the design and manufacture of tools and machines.


A. Mechanical

B. Civil
C. Electrical
D. Electronic 
37. The pilot light, the flue, heat exchanger fins and the pump are the components of ______________.


A. washing
B. refrigerator 


C. central heating

D. sewing 

38. _______________________ is the flow of electricity.


A. Force

B. Wire
C. Current
D. Spring

39. In the washing machine, _____________________ controls the flow of water into the machine.


A. heater

B. temperature sensor
C. motor
D. solenoid valves

40. Water freezes at ______________________ 0F and O0C.

A. 30

B. 31
C. 32
D. 33

41. If pressure is applied to the surface of an enclosed fluid, it is transmitted equally throughout 
the ____________________.                   

A. radiator

B. condenser

C. heat

D. fluid 
42. ______________________ is a long tube in the shape of a zigzag in structure of fridge.


A. Condenser

B. Evaporator
C. Compressor
D. Capillary tube

43. The temperature  ______________________  measures the water temperature and signals it 
to the control unit.





A. level


B. sensor        
C. scale

D. the control 

44. _____________________ is the flow of heat through a substance. Actual physical contact is required for heat transfer to take place between two bodies by this means.


A. Convector

B. Conduction
C. Conductor

D. Convection

45. Unless the diverter valve is switched to central heating, the radiators will not ________________.


A. wet

B. cold
C. heat up

D. cool
46. Most gas central heating works on the “_______________________” system of heat transfer between water flowing through pipes.
   

A. cold


B. cool
  

C. wet      
D. hot
47. The compressor compresses the gas so that it __________________________.


A. cools down

B. cools up
C. heats down
D. heats up

48. Unless mild steel is painted, it will ______________________.





A. correct


B. column

C. corrode 
D. carrot 

49. _______________________ is that branch of science dealing with the mechanical action of heat. 


A. Thermodynamic

B. Thermoduric
 C. Thermo cycle
D. Thermostatic
50. If a force is applied to a _______________________ fixed at one end, it extends in proportion to 
the force.


A. radiator

B. loop
C. spring
D. condense
The End of the Test
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