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MULTIPLE CHOICE: (Chọn câu trả lời đúng nhất điền vào phiếu bài làm. Mỗi câu đúng được 0,2 điểm)

	1
	A
	B
	C
	D
	6
	A
	B
	C
	D
	11
	A
	B
	C
	D
	15
	A
	B
	C
	D
	21
	A
	B
	C
	D

	2
	A
	B
	C
	D
	7
	A
	B
	C
	D
	12
	A
	B
	C
	D
	17
	A
	B
	C
	D
	22
	A
	B
	C
	D

	3
	A
	B
	C
	D
	8
	A
	B
	C
	D
	13
	A
	B
	C
	D
	18
	A
	B
	C
	D
	23
	A
	B
	C
	D

	4
	A
	B
	C
	D
	9
	A
	B
	C
	D
	14
	A
	B
	C
	D
	19
	A
	B
	C
	D
	24
	A
	B
	C
	D

	5
	A
	B
	C
	D
	10
	A
	B
	C
	D
	15
	A
	B
	C
	D
	20
	A
	B
	C
	D
	25
	A
	B
	C
	D




1.  _______________ is not an equipment in engineering.
     A. Calendar       B. Crane       C. Pump         D. Turbine
2. ___________ is a person whose job involves designing and building engines, machines, roads, bridges, etc.
		A. Engineering		B. Engineer
		C. Engineerer		D. Engineeror	
[bookmark: OLE_LINK3][bookmark: OLE_LINK4]3. A liquid is heated, it changes to a ________________ .
	A. iron          B. liquid         C. solid        D. vapour 
4. The liquid turns to vapour in the _________________.
		A. Condenser		B. Evaporator
		C. Compressor		D. Capillary tube
5. Engineering is not based on principal on ___________.
		A. physics		B. chemistry
		C. mathematics		D. literature
6. ________________ engineering deals with the design 
and manufacture of tools and machines.
		A. Electrical		B. Electronic	
		C. Mechanical		D. Civil 
[bookmark: OLE_LINK5][bookmark: OLE_LINK6]7. Electrical engineering includes__________ generating, electrical installation, lighting... 
		A. electricity 			B. electrical 
		C. electronic		D. electronics
[bookmark: OLE_LINK9][bookmark: OLE_LINK10]8. Two branches of engineering include both electrical and __________.      A. electronic	            B. aeronautical
	                        C. mechanical	            D. marine
9. All _______________ receive hot water directly from the boiler.                 A. thermostats	            B. radiators
	                       C. pumps	            D. flues
10. ______________ engineering describes engineering 
work performed by civilians for non-military purpose.
		A. Electrical		B. Electronic 
		C. Mechanical		D. Civil 
11. _____________ is the process of extracting coal and 
other materials from under the ground.
		A. Mining		B. Boiling
		C. Evaporating		D. Heating
12. A _______________ is any physical substance which keeps its shape even when not contained.
     A. solid          B. vapor           C. water        D. fluid
[bookmark: OLE_LINK21][bookmark: OLE_LINK22]13. A gas is cooled, it changes to a ________________ .       .   A. iron            B. liquid           C. solid         D. vapour
14. R12 has a very low boiling point: ________________.
[bookmark: OLE_LINK23][bookmark: OLE_LINK24]	A. 29°C         B. - 29°C         C. 29° F      D. -29°F
15. The compressor is switched on and off by a ________.
		A. thermostat	B. condenser
		C. radiator 		D. boiler  
16.__________ engineering includes marine, automobile, aeronautical, heating and ventilating, and others.              .	
	A. Electrical	B. Civil
	   C. Mechanical	D. Electronic
[bookmark: OLE_LINK91][bookmark: OLE_LINK90]17. As the warm gas passes through the condenser, it ___________ the surroundings and ____________ down.
[bookmark: OLE_LINK89][bookmark: OLE_LINK84] 	A. cool, heat	B. heats, cools
	C. cools, heats 	D. heat, cool
18. We can use “___________” to link an action and the limit of that action.            A. as                 B. until         
                                           C. after             D. when
19. As the liquid passes from the narrow capillary tube to the larger tubes of the evaporator, the pressure quickly ______________.             A. rise          	B. drop         
	                             	C. rises      	D. drops
20. Producing steel using the Bessemer process is one of the best-known __________________ processes.
		A. industry	B. industrious
		C. industrialize	D. industrial
21. Electronic engineering ___________ communications and equipment.
	A. are concerned with	B. deals with 
	C. is concerned of	D. is the concern with
22. Planes are ______________________ aeronautical.
	A. concerned of                     B. concern with			
	C. the concern with                D. the concern of
23. __________________ the system is switched on, 
cold water passes through a heat exchanger in the boiler.
      		A. When         	B. After          
		C. Until     	D. Before  	
24. Pilot light: - to ___________________ the boiler.
         A. ignite         B. cut            C. cool         D. cold
25. ________________: - to provide air for combustion; 
to allow exhaust gases to escape.
		A. Flue		B. Thermostat
		C. Burner		D. Pump
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[bookmark: OLE_LINK37][bookmark: OLE_LINK38]26. ________________: - to circulate water round 
the system.             
	A. Flue	  B. Thermostat
		C. Burner	  D. Pump
27. In conventional boilers, water _______________ 
by gas burners.           
	A. heats	  B. is heat
	   C. is heated	  D. is hot
28. The heat exchanger is made of tubes of cast iron or copper, which _________________ corrosion.
		A. resist		B. resists
		C. resisting		D. resisted
29. The last stage in operating sequence of gas central heating is cold water from _______________ returns to the boiler.             
	A. the loop	     	B. thermostat	
	   C. the radiators 	 D. heat exchanger
30. ________________ the water passes through 
the radiators, the water returns to the boiler.
		A. As	B. Until
		C. After	D. When 
31. ______________ the hot water flows through 
the radiators, the hot water loses heat.
		A. As	B. When
		C. After	D. Until
32. Solids can be ________________ easily.
		A. distributed	B. circulated
		C. piped 	D. pumped
[bookmark: OLE_LINK7][bookmark: OLE_LINK8]33. A typical system __________ a boiler, a network of pipes, a feed, an expansion tank, radiators and a hot water storage system.
		A. is included	B. are included
[bookmark: OLE_LINK1][bookmark: OLE_LINK2]		C. includes	D. including
34. If a gas expands, it _______________. 
		A. cooler	B. coolest
		C. cool up	D. cool down 
35. The other loop of the circuit passes to the _______________, which  provide room heating.
		A. radiators	B. radio
		C. boiler	D. cylinder
36. A thermostat located in the boiler causes the gas control valve to _________________ when the water temperature reaches the pre-set level.
		A. shut in	B. shut off
		C. shut out	D. shut down	
[bookmark: OLE_LINK39][bookmark: OLE_LINK40]37. We can use “_________________” to link two 
connected actions happening at the same time.
     A. as           B. until           C. after           D. when	
[bookmark: OLE_LINK15][bookmark: OLE_LINK16][bookmark: OLE_LINK13][bookmark: OLE_LINK14]38. We can use “___________________” to link 
an action and the limit of that action.
		A. as	B. until
		C. after	D. when
39. A gas is compressed, it _________________. 
		A. heats	B. cool down
		C. cool	D. heats up
40. The gas cools down in the _______________.
		A. compressor	B. heat exchanger
		C. condenser	D. evaporator.
[bookmark: OLE_LINK17][bookmark: OLE_LINK18]41. The compressor compresses the gas so that it ___________.    A. cools down	         B. cools up
		               C. heats down	         D. heats up
42. Refrigeration is based on __________ principles.
		A. 1             	B. 2             
		C. 3           	D. 4
[bookmark: OLE_LINK11][bookmark: OLE_LINK12]43. Refrigeration preserves food by ______________
its temperature.
		A. low	B. increase
		C. lowering	D. increasing
44. The refrigeration process begins in the ________.
		A. condenser	B. evaporator
		C. compressor	D. capillary tube
45. ______________ is a long tube in the shape of 
a zigzag in structure of fridge.
		A. Condenser	B. Evaporator
[bookmark: OLE_LINK19][bookmark: OLE_LINK20][bookmark: OLE_LINK103][bookmark: OLE_LINK104]		C. Compressor	D. Capillary tube
46. Newer refrigerants such as _________________ 
are gradually replacing  R12.
[bookmark: OLE_LINK25][bookmark: OLE_LINK26][bookmark: OLE_LINK27]		A. KLEA 134	B. KLEA 134a
		C. KLEA 341	D. KLEA 341a
47. The second stage in the refrigeration is the gas passes through the __________________.
		A. compressor	B. evaporator
		C. condenser	D. capillary tube
48. A force is applied to a body, there is an equal 
and opposite __________________.
		A. action	B. acting
		C. act	D. reaction
[bookmark: OLE_LINK30][bookmark: OLE_LINK31]49. ______________ leaving the condenser has to 
flow down a very narrow tube.
		A. Solid	B. Vapour
		C. Gas	D. Liquid
[bookmark: OLE_LINK28][bookmark: OLE_LINK29]50. If a current passes through a wire, it sets up __________________ around the wire.
		A. the fluid	B. a magnetic field 
		C. a liquid 	D. a current


   		 
	 

 



