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1. ______________is then sucked back into the compressor and the refrigeration process begins again.
	A. Cold vapour	    C. Cold liquid
	B. Warm vapour	   D. Warm liquid
2. Most washing machines use 83 rpm for _____________.  
	A. spinning        B. washing        C. mixing		
	D. distributing the load before spinning  
3. If it rains, the grass _____________ wet.
	A. gets      B. got      C. to get     D. getting
4. For ammonia refrigerating systems, the tubes of a shell and tube condenser are made 
of ________________.
	A. cooper		C. aluminum
	B. steel	D. brass
5. A thermostat regulates temperature so that the food is not ________________.
	A. frozen		C. freeze
	B. over-frozen		D. froze
6. The cold vapor ____________ heat from 
the fridge.       A. absorbed	         C. to absorb
	            B. absorbs	D. absorbing 
7. As the liquid passes from the narrow capillary tube to _____________ tubes of the evaporator         A. narrow               C. larger
                          B. large	              D. big 
8. The temperature sensor is a type of _________ which fits inside the washer drum.
	A. clock		C. thermometer
           B. fan		D. watch
9. If you heat ice, it ________________.
	A. to melt		C. melting
	B. melts 		D. melted
10. If the water temperature is too low, the control unit will switch on _____________.
	A. the boiler	C. the heater	
	B. the burner	D. the drum	
11. The capillary tube is not used in large capacity refrigeration systems because _____.            .         A. it is made of copper		
          B. capacity control is not possible
  C. cost is too high
  D. required pressure drop cannot be achieved	
12. Lowering the pressure around a liquid helps it to _____________.
     		A. boil        		B. steam	
		C. vapor     		D. cool
13. Most washing machines use 100 rpm for __________. 
     A. spinning          B. mixing       C. washing	  	
     D. distributing the load before spinning
14. If a current passes through a wire, ______.
   A. it is transmitted equally throughout fluid	
   B. it sets up a magnetic field around the wire	
   C. it changes to a liquid
   D. a current is induced in the wire
15. To keep the refrigerator at a constant low temperature, heat must be _______________ from the inside of the cabinet to the outside.
	A. transfer		C. transferring
	B. transfers	D. transferred
16. ________________ is a force shown by something in response to another force.
	A. Force		C. Current
	B. Reaction	D. Spring
17. Newer refrigerants which are less harmful to the environment, such as ___________, are gradually replacing R12.
		A. KLEA 134a		C. KLAE 134a
		B. KLEF 134b		D. KLAF 134b
18. The refrigeration process begins in the __________.
		A. condenser		C. compressor
		B. evaporator		D. capillary tube
19. ___________ is a long tube in the shape 
of a zigzag in structure of fridge.
		A. Condenser	
		B. Evaporator 
		C. Compressor
		D. Capillary tube
20. Plants die if they ________ enough water.
      	A. get	C. don’t get
	 	B. to get	D. getting
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21. ______________ is metal in the form of thin thread that is used to carry electric current.
	A. Force		C. Spring
	B. Wire	D. Current
22. If you ___________ water, it ___________ at 1000C.
	A. heat/ boils	C. heated/boiled
	B. heats/boils                D. is heated/boiled
23. The compressor compresses the gas so that it _________________.
	A. cools down	C. heats down
	B. cools up	D. heats up
24. Refrigerant has a very _______________ boiling point: -290C.
A. low		C. constant
B. high		D. average
25. ______________ is a piece of electrical equipment in which food is kept cold so that it stays fresh.
A. Washing machine        C. Refrigerator
B. Central heating            D. Air – conditioner
26. Refrigeration is based on ____________ principles.
	A. 1 	B. 2 	C. 3 	D. 4	
27. One common refrigerant is not a compound of ______________.
	A. carbon    	C. All are wrong
	B. chlorine 	D. All  are correct
28. ______________ is the flow of electricity.
	A. Force 		B. Wire
	C. Current 		D. Spring	
29. ______________ is circulated around the fridge, where it undergoes changes in pressure and temperature and changes from a liquid to a gas and back again.
	A. Refrigerant	     B. Refrigeration
	C. Refrigerator	     D. Refrigerater
30. _____________ is a device that cools gas in order to change it into liquid.
	A. Compressor 		B. Condenser	
	C. Capillary tube 		D. Evaporator
31._____________the warm gas passes through the condenser, it heats the surrounding and cools down.             A. As 	                B. When 
                                 C. After             D. Until
32. ___________ leaving the condenser has to flow down a very narrow tube.
	A. Solid     B. Vapour      C. Gas    D. Liquid	
33. ______________ is a device in the fridge 
that regulates temperature so that the food is not over-frozen.
		A. Thermostat		C. Compressor
		B. Button		D. Cylinder
34. _______________ is not the component of the washing machine.
	A. Condenser	    C. Control unit
	B. Door lock	    D. Shock absorber
35. If a gas ______________, it heats up.
	A. compresses		C. expands
	B. is compressed		D. is expanded
36. If a wire cuts a magnetic field, _________.
    A. a current is induced in the wire. 		
    B. it extends in proportion to the force.
    C. it heats up
    D. it sets up a magnetic field around the wire.
37. The gas condenses back into __________.
	A. solid 		B. liquid	
	C. vapour 		   D. fluid
38. Refrigeration preserves food by _________
its temperature.
    	A. lower      		B. lowers    
	C. lowering    		D. low
39. In the washing machine, _________ pumps water out of the drum.           
   A. absorber      B. motor      C. pump    D. fan	     
40. _____ rotates the drum in washing machine.	
	A. Heater		C. Fan
	B. Motor		D. Solenoid valves




