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MULTIPLE CHOICES Choose the word or phrase that best completes the sentences (10 ms)

1. The movement of the spot across the screen is controlled by __________.
A. the line scan signal           B. the line signal                C. All are correct.                  D. All are wrong.

2. When the spot reaches the bottom of the screen, 

it is blanked and moved rapidly back to the  ___________ of the screen.             

       A. top        B. bottom         C. middle       D. end
3. What controls data going in and out of the computer ? ________      A. O/I         B. O/O               .                                        C. I/O
D. I/I

4. The frame must be scanned at least __________ times per ____________to prevent the screen from flickering.

  
A. forty, second             B. forty, minute    
C. fourteen, second        D.  fourteen, minute

5. The invention of the  ________ meant that much  smaller, low-powered devices could be developed.

A. capacitor
B. transistor         

C. resistor                
D. thermos
6. Each ____________ is marked with colours to indicate its value.


A. transistor 
B. resistor            

C. thermos                     D. capacitor


7.  The light bulb _________ by Thomas Edison.


A. is invented
B. was invented


C. invent
D. invents

8. This problem ____________ by his father.

   A. solve    B. solves    C. can be solved   D. solved

9. The apples ____________ by her sister.


A. are being eaten   
B. eats  


C. are eating    
   D. eat   

10. Electronics engineers are required to design and service __________, including control panels.


A. industry circuits
B. circuits

C. industrial circuits
   D. All are wrong.
11. You can _________ sound on tape or disc.
 A. rectify      B. record     C. suppress     D. conduct

12. HDTV consists of __________ dots. 

A. 450,000

B. 460,000

C. 470,000

D. 480,000

13. HDTV offers you _________-dimensional sound, as it uses more speakers than today’s sets.

      A. two          B. three         C. four        D. five     

14. What would be the effect of making resistors with a make higher tolerance ? – The price would be ___________.      A. lower               B. cheaper 
   

                                  C. higher
   D. middle

15. _________ uses 1,250 lines per frame.


A. existing TV
B. HDTV

C. TV set
D. All are correct.

16. __________ the news ___________ by you ?

         
A. Have, hear
               B. Have, been heard

         
C. Had, hear
               D. Has, been heard

17. The sound of ________ is mono and stereo.

A. existing TV      B. HDTV      C. HTV    D. SCTV
18. For HDTV the width/height ratio of the screen has been changed from _______ to ________.       
A. 4:3, 16:3         
B. 4:6, 16: 3         C. 4:6, 16:6         
D. 4:3, 16:9

19. MSI is the abbreviation of __________ .

A. medium-scale integrate  

B. medium-scale integration

C. medium-scale integrated

D. All are correct.

20.  If I had known your address, I _______ you a postcard.       A. will send                  B. had sent
           


 C. would have sent      D. would send

21. CPU controls the rest of the system and performs all the arithmetic and ____________ operations on the data.     A. logical        B. logic

                             C. logistic       D. logistical  
22. The screen of HDTV is ___________ .

     A. flat        B. curve       C. round
      D. square

23. The size of HDTV is ________ centimeters.

    A. 60-70     B. 100-125   C. 105-125   D. 125-135


24. Once equipment ______________, it needs 
to be commissioned.

A. install                           B. installation    
  C. installs

      D. is installed

25. It’s used for measuring very small current. It’s called a ___________ .

A. microammeter
B. milliammeter          C. multimeter         
D. All are correct.
26. It’s used to find buried metal. It’s called _____.

A. metal detector              B. milliammeter           
C. multimeter           
      D. All are correct

27. There is a wide range of ___________ work required, for example, installing exchanges, LANs, and medical equipment.    


A. install
B. installing 
   

C. installation
D. installed

28. HDTV provides the viewer with more ________ than are offered by today’s television sets.

A. unrealistic images              B. realistic images                C. All are correct.             
      D. All are wrong.

29. __________ electronic equipment has to be maintained to a very high standard with rigorous checks at set intervals.          

A. Defence                     B. Computing                  C. Aircraft                      D. Leisure products

30. ________ is built up gradually by moving a spot of light across and down a screen in a raster pattern. 

A. A television picture     B. A computing                                           C. Defence                        D. Leisure products

31. The viewing range of HDTV is ______ degrees.


A. 10           B. 20          C. 30          D. 40

32. The radio ___________ a tuner, a detector, and 
AF amplifier. 

A. consists of
B. is composed of

C. All are correct.
D. All are wrong.

33. A wider range of frequencies can be used to transmit each ________ channel.
      A. VTV
  B. HTV        C. SCTV      D. HDTV

34. To allow the video signal to be transmitted using a smaller range of frequencies, each frame is transmitted in two separate _________, known as field.                A. half       
       B. have                      

C. halves       
       D. had

35. The scan rate must be greater than _______ Hz, because a lower scan rate would cause the screen to flicker.        A. 30
  B. 40          C. 50         D. 60

36. The sync pulses are added to the __________ to ensure that the TV camera and TV receiver start a new line and frame at the same time.

A. video film   
   B. video tape
C. video signal  
   D. All are correct.   

37. The rapid movement of the spot back across the screen to the start of the next line is called _______.

   
A. scan   

   B. signal   

C. video signal   
   D. flyback
38. A new car _____________ by Alan.

      A. buy     B. bought    C. is buy    D. was bought
39. Existing European TV system uses __________ lines to ensure a good quality picture.         

       A. 605          B. 615           C. 625         D. 635 

40. The optional viewing distance for HDTV is _________ times the height of the screen compared with present TV.          A. one              B. two           
       


 C. three            D. four

41. The build-up of the screen happens so quickly that the eyes see only a ___________.

    A. to complete picture         B. completed pictures     

    C. incomplete image            D. complete picture

42. The small _________ provides some permanent

storage and the ___________ is used for temporary storage.      A. CPU, RAM                B. RAM, ROM                                          .                  C. ROM, RAM
          D. I/O



43. It’s used to master down different recordings to make a master tape. It’s called a _________.

A. mixer desk

    B. mixing desk

C. All are correct
    D. All are wrong.

44. ___________ is used to transfer data between all the units.       A. Address bus         B. Control bus   

               C. Data bus              D. Data

45. _________ is used to send control signals from the CPU to the other units.

A. Address bus
    B. Control bus           
C. Data bus               
    D. All are correct.

46. Sets of connectors known as buses are used to carry the ___________ between each unit.


A. outside signals
    B. signals         

C. internal signals           D. All are correct.

47. It’s used to check the logic levels in the pins of ICs. It’s called a(n) ___________.

A. logic probe

    B. logic prober    

C. unlogic probe             D. unlogic prober

48. It’s used as part of a burglar alarm to detect movement. It’s called a(n) __________.

A. motion sensor
  B. promotion sensor                 C. emotion sensor         D. motivation sensor

49. ____________ are now used to control many household items such as washing machines …
        A. Microprocessors            B. Microwave      
        C. Microphones                  D. Microcomputers          

50. In a radio the tuner _________ to the detector.

A. is connected to   
B. is linked to


C. All are wrong.  
D. All are correct.
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