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MULTIPLE CHOICES       Choose the word or phrase that best completes the sentences ( 10 ms )

1. A wider range of frequencies can be used to transmit each __________________ channel.

      
A. VTV               
B. HTV           

C. HDTV
D. SCTV

2. The flowers __________ in this garden.


A. can planted   
B. plants


C. will be planted   
D. planting
3. The frame must be scanned at least forty times per second to ____________ the screen from flickering.    
A. pulse          

B. cancel          

C. transmit
  
D. prevent

4. To allow the video signal to be transmitted using a range of frequencies, each frame is transmitted in two separate _____________, known as field.      
     

      A. half         B. have         C. halves        D. had

5. The scan rate must be greater than ________ Hz because a lower scan rate would cause the screen 
to flicker.       A. 30
   B. 40         C. 50        D. 60

6. There is a wide range of ____________ work required, for example, installing exchanges, LANs, and medical equipment.    

A. installation              
B. install 
         C. installing
D. installed

7. HDTV provides the viewer  with more ________ images than are offered by today’s TV sets.

  
A. realistic          
B. unrealistic          C. All are correct.          D. All are wrong.

8. ____________ electronic equipment has to be maintained to a very high standard with rigorous checks at set intervals.     

A. Aircraft                     B. Computing                        C. Defence                   
D. Leisure products

9. The viewing range of high definition television is  ____________ degrees.

        A. 10     
     B. 20         
C. 30            D. 40
10. Sets of connectors known as buses are used to carry the ______________ between each unit.

           A. outside signals
   B. signals         

           C. internal signals           D. All are correct.

11. It’s used to check the logic levels in the pins of ICs. It’s called a(n) _____________.

A. logic probe
B. logic prober    
              C. unlogic probe             D. unlogic prober

12. It’s used as part of a burglar alarm to detect movement. It’s called a(n) _____________.

   A. motion sensor

  B. promotion sensor                   C. emotion sensor               D. motivation sensor

13. It’s used for the transmission of RF signals. It’s called a(n) _________.   A. resistor          B. antenna      

                            C. capacitor       D. serial          

14. This problem _________ by my father.
  A. solve     B. solves    C. can be solved   D. solved

15. The sync pulses are added to the _________ to ensure that the TV camera and TV receiver start a new line and frame at the same time.
A. video film        
B. video      
           C. video signal     
D. All are correct.

16. What controls data going in and out of the computer ? ________      A. O/I         B. O/O               .                                        C. I/I
D. I/O
17. _________ is the rapid movement of the spot back across the screen to the start of the next line.
   
A. Scan         
B. Image        


C. Signal      
D. Flyback
18. Existing European TV system uses __________ lines to ensure a good quality picture.      

       A. 605         B. 615           C. 625          D. 635 

19. The optional viewing distance for HDTV is __________ times the height of the screen.  

    A. one          B. two           C. three           D. four
20. The build-up of the screen happens so quickly that the eyes see only a ________________.

       A. completes picture          B. complete picture        

       C. incomplete image          D. complete pictures
21. The small _________  provides some permanent storage and the ___________ is used for temporary storage.       A. CPU                    
B. RAM, ROM                        .                   C. ROM, RAM       
D. I/O

22. CPU is used to control the system, perform  all arithmetic and ___________ operations on the data.

   
A. logic     
B. unlogical      


C. logical      
D. unlogic

23. _____________ is used to transfer data between all the units.   A. Address bus       B. Control bus   



           C. Data bus            D. Data

24. __________ is used to send control signals from 
the CPU to the other units.


A. Address bus
B. Control bus           
C. Data bus               
D. All are correct.

25. The light bulb ___________ by Thomas Edison.



A. is invented
B. was invented



C. invent
D. invents
26. The central processing unit is a __________. 

A. microprocessor      
B. processor        


C. microphone        
D. process

27. The decision-making circuits used in modern computers are mainly composed of combinations of digital switching circuits known as ____________.

         
A. logical gates
B. logic gates

C. unlogic gates                D. unlogical gates

28. For HDTV the width/height ratio of the screen has been changed from _____________ ( as in conventional TV) to _____________.       

A. 4:3, 16:3        
B. 4:6, 16: 3         
C. 4:6, 16:6           
D. 4:3,16:9

29. HDTV consists of ______________ dots.

A. 460,000    B. 470,000    C. 480,000    D. 490,000

30. This cake ____________ by my mother.

   A. make       B. makes     C. was made     D. made
31. The movement of the spot across a TV screen is controlled by the line ___________.

          
A. scan signal          
B. signal scan                  
C. All are correct.             D. All are wrong.

32. When the spot reaches the bottom of the screen, it  is  blanked  and  moved  rapidly  back  to  the ________________ of  the screen.             

       A. top         B. bottom       C. middle       D. end

33. In the USA, the more generic term ATV, Advanced Television, has been __________.

   A. refuse    B. refused      C. adopted   D. adopting
34. The frame must be scanned at least __________ times per second to prevent the screen from flickering.     
       A. four               B. fourteen       

                               C. forty              D. four hundred
35. The  invention  of  the ____________ meant 

that much smaller, low-powered devices could be developed.        A. capacitor
       B. transistor         
               .                         C. resistor             D. insulator
36. Each __________  is marked with colours to indicate its value.   A. transistor
B. resistor            

       C. insulator           D. capacitor

37. The apples ________________ by her sister.


A. are being eaten   
B. eats  

C. are eating    
D. eat   
38. ___________ the news ____________ by you ?

         
A. Have, hear                 B. Have, been heard

         
C. Had, hear
               D. Has, been heard
39. The radio ______________ a tuner, a detector, 

and an AF amplifier.


A. consists of     
B. is composed of


C. All are correct  
D. All are wrong.
40. ___________ uses 1,250 lines per frame.

      A. VTV       B. SCTV        C.  HDTV     D. HTV                

41. It’s  used  to  find  buried  metal. It’s called ________ .   A. metal detector     B. milliammeter           
         C. multimeter           D. All are correct.
42. MSI is the abbreviation of   ________________.
 
A. medium-scale intergrate       


 
B. medium-scale intergration       


C. medium-scale intergrating  

D. All are wrong.

43. TTL is the abbreviation of  _______________ .

 A. transistor-transistor logic  
       C. All are correct.   
 B. transistor-transistor logical      D. All are wrong.
44. The screen of HDTV is __________________.      

    A. square      B. flat        C. curved       D. round

45. Once equipment _______________, it needs 
to be commissioned.    A. install    
  B. is installed     
                                     C. is install    
  D. installing
46. You can _____________ sound on tape or disc.                  .  A. rectify     B. record      C. suppress   D. conduct


47. The size of HDTV  is ___________ centimeters.

A. 60-70    
 
B. 100-125  

C. 105-125  

D. 125-135

48. HDTV offers you _____________-dimensional sound, as it uses more speakers than today’s sets.

      A. two            B. three          C. four         D. five     

49. What would be the effect of making resistors with a make higher tolerance ? – The price would be  __________.      A. lower            B. cheaper 
        .                                C. higher
           D. taller
50. The tuner ____________ the detector.

A. is connected to   
    B. is linked to

C. All are correct.  
    D. All are wrong.
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