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MULTIPLE CHOICES     Choose the word or phrase that best completes the sentences (10ms)

1. _________________ is invented in 1947.       


A. Transistor
  B. Resistor         
C. Transmit           
  D. All are correct.      

2. Electronics began at the start of the ___________ century with the invention of the vacuum tube.
 

A. nineteenth

     B. twentieth         
C. twenty-first        
     D. twenty- second

3. It was not until 1958 that ___________ began with the development of integrated circuits on silicon chips.

A. microelectronics
B. microphone                   C. microcomputer        
D. All are wrong.

4. The light bulb ____________ by Thomas Edison.



A. is invented
B. was invented



C. invent
D. invents

5. ____________ is used in radios, televisions, record players, and tape recorders.


 A. Transformer
B. Vacuum tube                C. Thermistor
D. Capacitor

6. This problem _________________.

     A. solve   B. solves   C. can be solved   D. solved
7. The apples _________ by her sister.

A. are being eaten   B. eats  C. are eating    D. ea
8. SLSI is the abbreviation of _______________.

    
A. super-large-scale intergate
 
B. super-large-scale intergation        
C. super-large-scale intergated         
D. All are correct.

9. ___________ the news ___________ by you ?

         
A. Have, hear                 B. Have, been heard

         
C. Had, hear
               D. Has, been heard

10. There are ___________ common families of logic ICs used in computers.

        A. two
     B. three
   C. four        D. five
11. VLSI is the abbreviation of ________________.

      
A. very large-scale intergrate
 
B. very large-scale intergration

C. very large-scale intergrated    
D. All are correct.

12. TV  sets  are  manufactured  with  each  set consisting of up to seven individual ____________.


A. model
B. modern             
C. modules
D. modest
13. The decision-making circuits used in modern computers are mainly composed of combinations of digital switching circuits known as ____________.

         
A. logic gates
B. logical gates

C. unlogic gates                D. unlogical gates

14. Sound quality of HDTV is superb, thanks to digital multitrack __________.
A. transportation   
B. transfer

C. transmissions   
D. All are correct.

15. Picture quality of HDTV is excellent, clear, and without ________.   A. flicker              B. flicking


         C. click
               D. hacker
16. The tuner ____________ the detector.


A. is connected to  
B. is linked to


C. All are correct.    
D. All are wrong.

17. Once a week, the house ___________ by Mary.

  A. clean    B. cleans   C. cleaned    D. is cleaned

18. ___________ are now used to control many household items such as dishwashers …

     
A. Microprocessors          B. Microcomputers


C. Microphones                D. Microwave
19. The radio consists of a tuner, a detector, and 
an __________.      A. amplifier  
   B. amplify   
                     .                               C. AF amplifier  
   D. amplified

20. Computers _____________ data.  


   A. conduct      B. emit       C. process      D. record

21. The aim of high definition television (HDTV) is to provide the viewer with more _____________ images than are offered by today’s television sets.  
  

  
A. real      

B. realistic      
C. unreal     

D. unrealistic 

22. HD picture consists of ___________ lines and 
is composed of ____________ times as many dots.


A. 1250, one 
B. 1520, two          

C. 1520, three
D. 1250, four
23. For HDTV the width/height ratio of the screen has been changed from __________ to ________.


A. 4:3,16:6 
B. 4:3,16:7          
C. 4:3,16:8
D. 4:3, 16:9
24. The optimal viewing distance for ___________ is three times the height of the screen compared with seven times the present television.    
    A. VTV        B. HTV        C. HDTV     D. SCTV 

25. TTL ICs use bipolar transistor to ____________ each gate whereas CMOS ICs use field effect transistor (FETs).       A. form
             B. formation

                                   C. formal
 D. format
26. The line scan signal controls the movement of the _____________ across a television screen.


A. spot      
B. flashlight     


C. All are correct.      
D. All are wrong.

27. There are ____________ lines used to build up a frame in present European television systems.

        A. 600          B. 615     
  C. 625         D. 635

28. If the frame is not scanned at least forty times per second, it ________.  A. flicking     B. flickers    
                                          C. flick     
    D. click

29. _________ is the rapid movement of the spot back across the screen to the start of the next line.


A. Flyback       
B. Playback    
C. Feedback    
D. Clicking
30. Electronics engineers are required to design and service industrial circuit, including __________.

         A. control panels                B. control panel

         C. All are correct.               D. All are wrong.

31. The books ____________ by her sister.

  A. buy    B. were bought    C. are buying    D. buys  
32. ROM is the abbreviation of ________________.
    A. Read On Memory         B. Read Only Memory          

    C. All are correct.              D. All are wrong.
33. The _________ or __________ unit consists of one or more ICs, which are used to control the data going in and out of the computer.  


A. input, output        
B. gate, gate          C. All are correct.    
D. All are wrong.

34. ____________ is used to store programs and 

data temporarily.         A. RAM       
  B. CPU




C.  ICs

  D. ROM


35. Unlike the __________, the content of the ___________ is constantly changing, but it only operates while the computer is switched on.   


A. RAM, ROM      
B. ROM, RAM      
C. All are correct.    
D. All are wrong.

36. ____________ is used for transmission of RF.

 A. Antenna    B. Resistor   C. Capacitor     D. Serial

37. If you remove a file by a mistake, you can find 
 it in ____________.


   A. My Computer 
  B.  My Connection 
          .        C. Recycle Bin 
  D. My Documents

38. It’s used for protecting circuits from a surge in 
voltage. It’s called a  _______________ .


A. fuse                            B. surge fuse
 

C. All are correct            D. All are wrong.
39. Almost every large business organization, like banks and insurance companies, runs several local area networks (LANs). These require network manegers, _______________  and software support.


A. maintain         
B. maintaning                   
C. maintenance                 D. All are correct.

40.  CD-ROM disks can hold quite ____________ 

amounts of data.       A. small              B. large 
                                  C. low                 D. tiny 
41. The picture is displayed using ____________ per frame.             A. less dots
 B. less lines
      .                             C. more lines
 D. more dots

42. In Europe, the term _____________ is used.      

    A. HTV        B. HDTV       C.  SCTV       D. VTV

43. Computers use ______________ which contain a number of logic gates on one chip.


A. ICs        
B. Integrated circuits        C. All are wrong       
D. All are correct.

44. The number of components in an IC is indicated by its scale of ______________ .


A. integration                
B. integrated           
C. international              D. All are correct.

45. ______________ is used to send signals from the CPU which indicate the memory and I/O locations to be used.


A. Address book       
B. Address bus        C. Address card       
D. All are correct.

46. In the USA, the more generic term ATV, Advanced Television, has been ___________ .


A. canceled       
B. omitted       
  C. adopted       
D. All are correct.

47. Resistor labelled 5R6. It means ____________.  


A. 5.6 ohms     
B. 5.6 kilovolts                    C. 5.6 gigahertz
D. 5.6 megohms

48. A ____________ resistor is a resistor which you can vary or change by turning the control.

  A. various      B. vary       C. variable     D. Various 
49. A _________ is used to find buried metal.

A. detector   B. metal detector   C. Aerial  D. Serial
50. A ________ sensor is used as part of a burglar alarm to detect movement.  
 A. emotion    B. motions    C. motion    D.capacitor
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