REVIEW
1. Pilot light – to………… the boiler.
A.  ignite		B.  start to burn	C. burn	D. A and B are correct.	
2.  Heat exchanger fins – to increase the surface area in contact with water, which improves the ……….....
A. heating transfer	B.  transfer of heat	 C.  heat transfer		D.  All are correct.
3. ………… the system is switched on, cold water passes through a heat exchanger in the boiler.
A. When		B. As			C.  After			D. If
4. …………. the water passes through the heat exchanger, it becomes hotter and hotter ………… it reaches a pre-set level.
A. When/ as		.B As/ after		C. As/ until			D. When/ after
5. …………. the water is pumped to a diverter valve, it goes to the hot water cylinder or the radiators.
A. When		B. As			C. After			D. until
6. After the water passes through the radiators, it ……….. to the boiler.
A.  return		B.  returns		C. returned			D. to return
7. Most gas central heating .………. on the ‘wet’ system of heat transfer between water flowing through pipes.
A. work		B. works		C. working			D. worked
8. A typical system ..………. a boiler, a network of pipes, a feed, an expansion tank, radiators, and a hot water storage system.
A.  is included		B.  are included	C.  includes			D. is including
9.  In conventional boilers, water …………. by gas burners.
A.  heats		B.  is heat		C.  is hot			D. is heated
10. The flow of gas to the burner ______ by a valve (or valves) which can ______. by a time switch or by a boiler thermostat.
A. is controlled/ be operated			B. control/ operate	
C.  is operated/ be controlled			D. controlled/operate
11. Air ……….necessary for complete combustion and …………. supplied to the burners either from inside the house, or directly from outside through a balanced flue.
A. is/ are		B.  are/is		C.  is/ is			D.  are / are
12. Water ………….. through a heat exchanger above the burner.
A. circulate		B. circulating		C. circulated			D. is circulated
13. The heat exchanger is made of tubes of cast iron or copper, which ………corrosion.
A. resist		B. resists		C.  resisting			D.  resisted
14. After being …….. through a diverter or priority valve, water …… around either one of two loops of pipework, which act as heat exchangers.
A. pump / circulate				B. pumped / circulated	
C. pumped/ circulates				D. pumps / circulated
15.  If a gas …….., it heats up.
A. compresses		B.  compressed	C. is compressed		D. will be compressed
16.  If a force is applied to a body, ……………
A. it extends in proportion to the force.		B. there is an equal and opposite reaction.
C.  it sets up a magnetic field around the wire. 	D. a current is induced in the wire.
17. If a current passes through a wire,…………
A. it extends in proportion to the force.		B. there is an equal and opposite reaction.
C. it sets up a magnetic field around the wire. 	D. a current is induced in the wire.
18.  If a wire cuts a magnetic field,…………
A.  it extends in proportion to the force.		B. there is an equal and opposite reaction.
C.  it sets up a magnetic field around the wire. 	D. a current is induced in the wire.
19.  If pressure is applied to the surface of an enclosed fluid, ……..…
A.  it extends in proportion to the force.    	B. it transmitted equally throughout the fluid.
C.  it sets up a magnetic field around the wire. 	D. a current is induced in the wire.
20.  If a force is applied to a spring fixed at one end,…………………
A.  it extends in proportion to the force.     	B. it transmitted equally throughout the fluid.
C. it sets up a magnetic field around the wire. 	D. a current is induced in the wire.
21. Engineering is largely a practical………….. it is about putting ideas into action.
A. activity		B. an activity			C. the activity		D. activities
22. ………… engineering deals with making bridges, roads, airports, ect.
A. Mechanical		B.  Civil			C.  Electrical		D. Ventilating
23. …………….. engineering deals with the design and manufacture of tools and machines.
A. Mechanical		B. Civil			C. Electrical		D. Electronic
24. …….. engineering is about the generation and distribution of electricity and its many applications. 
a. Mechanical		B. Civil			C. Electrical		D. Ventilating
25. _________engineering is concerned with developing components and equipment for communications, computing and so on.
A. Mechanical		B.  Civil			C.  Electrical		D. Electronic
26. _______ engineering includes marine, automobile, aeronautical, heating and ventilating, and others. 
A. Mechanical		B. Civil			C.  Electrical		D. Electronic
27. Electrical engineering includes electricity generating, …….. installation, lighting, ect.
A. Mechanical		B. Civil			C. Electrical		D. Electronic
28.  Mining and medical engineering …………… partly …………  mechanical and partly to electrical.
A. belong/ to	B. belong / of		C. belongs/ to 			D. belongs/ of
29.  …………..: Cars, train, ships, and planes are all products of mechanical engineering. Mechanical engineers are also involved in support services such as roads, rail track, harbours and bridges.
A. Civil		B. Transport		C.  Medical engineering	D.  Food processing
30. 22______: Mechanical engineers design, develop, and make the machines and the processing equipment for harvesting, preparing and preserving the foods and drinks that fill the supermarkets.
A.  Civil		B.  Transport		C. Medical engineering	D. Food processing
31. _______: Body scanners, X-ray machines, life-support systems, and other high-tech equipment result from mechanical and electrical engineers combining with medical experts to convert ideas into life-saving and preserving products.
A.  Civil		B. Transport		C. Medical engineering	D. Food processing
32. ________: Electrical engineers provide all the services we need in our homes and places of work, including lighting, heating, ventilation, air-conditioning, refrigeration, and lifts.
A. Energy and power 	B.  Building services	C.  Medical engineering	D.  Food processing
33. _______: Electrical engineers are concerned with the production and distribution of electricity to homes, offices, industry, hospitals, colleges and schools, and the installation and maintenance of the equipment involved in these processes.
A.  Energy and power B. Building services	C. Medical engineering	D. Food processing
34.  I work in a _______ I’m responsible for turbine maintenance.
A.  food processing	B. energy and power	C. power station		D. building services
35.  I work shifts: midnight ________ eight o’clock this month.
A.  from		B. on			C. at				D. to
36.  I design _______ They give doctors far more information than X-rays and there’s no risk to the patient pictures	B. photo machines	C. body scanners		D. X-ray machines
37. I work on jet engines. Onboard computers record readings every five hours and every twenty-five take-offs. This information allows us …………. servicing before defects or reduction in performance occur.
A. carry out		B. carrying out		C. to carry out			D. carried out
38. I’m working with the architects of a new hospital. Getting the ………….. right is important. I have to make sure that the working environment will be comfortable for the patients and staff.
A. generation	B.  refrigeration		C. lighting	D. heating and ventilation
39. [bookmark: _GoBack]Safety is very important in my job. Everything must be earthed to make sure that no one gets a __________
A.  shock		B. short			C. shorts			D. shocks
40.  For refrigeration process, the liquid turns to vapour in the ………...
A. condenser		B. evaporator		C.  heat exchanger	D. capillary tube
41. For the refrigeration process, the gas cools down in the ………………
A. condenser		B.  evaporator		C. heat exchanger	D. capillary tube
42.  The warm gas passes through the condenser, where it………………
A.  undergoes changes in pressure and temperature.	B. the high pressure is maintained.
C.  expands and cools.					D. heats the surroundings and cools down.
43. The refrigerant circulates around the fridge, where it …………………
A. undergoes changes in pressure and temperature.	B. the high pressure is maintained.
C. expands and cools.					D. heats the surroundings and cools down.
44. ____________is a tube with a very small diameter bore.
A. Capilary tube	B. Condenser		C. Refrigerant		D. Pilot light
45. ___________a unit where vapour is converted back into a liquid. 
A. Capilary tube	B. Pilot light		C. Condenser		D. Refrigerant
46. _____________a valve used in central heating to redirect the flow of hot water from radiators to water heating and vice versa. 
A. Pilot light		B.  Condenser		C. Refrigerant		D. Diverter valve
47. ____________a unit in which a liquid is converted into a vapour
A. Evaporator		B. Refrigerant		C. Compressor		D. Pilot light
48. ________________: the part of a boiler where the water is heated.
A. Diverter valve 	B. Heat exchanger 	C. Capillary tube	D. Pilot light
49. ____________: a small flame used to ignite the main burners  in a gas-fired heating boiler.
A.  Diverter valve 	B. Heat exchanger 	C. Capillary tube	D. Pilot light
50. ______________a substance which changes easily from a liquid to a gas and which can be used in refrigeration to remove heat energy and transfer it to the surroundings.
A. Refrigerant 		B. Condenser		C. Refrigerator		D. Pilot light
51. Most ……………… in the home have some sorts of control. 
A. device		B. devices		C. equipment		D. equip
52. For example, you can control the volume of a TV by using a ________ control. 
A. remote 		B. far			C. distance		D. mote
53. The _______ can be any movement or any change in the environment. For example, a drop in temperature may cause a heating system to come on.
A. input		B. output		C. control		D. signals
54. The ________ may change the size of the output (for example, adjusting the sound of a TV). Often this involves changing one kind of input into a different kind of output. For example, opening a window may set off a burglar alarm.
 A. input		B. output		C. control		D. signals
55. __________ can be of many kinds. An alarm system may ring a bell, flash lights, and send a telephone message to the police.
A. Input		B. Output		C. Control		D. Outputs
56. Most control systems are closed loops. That means they incorporate a way of checking that the ________ is correct. In other words, they have feedback. 
A. input		B. output		C. control		D. signals
57. The control system of a modern washing machine has to take into account several different _________.
A. factor		B. factors		C. fact			D. facts
58. These are door position, water level, water temperature, wash and spin times, and__________. Most of them are decided when you select which washing program to use.
A. drum speed	B. speed drum	C. drum speeds	D. speed drums
59. The _________is the heart of the system. 
A. control unit 	B. door position	C. water level		D. water temperature
60. It receives and sends out signals which control all the activities of the machine. It is also capable of diagnosing faults which may occur, stopping the program, and informing the service engineer what is wrong. It is a small, dedicated computer which, like other computers, uses the language of logic.  It refers to the _____________.
A. control unit 	B. door position	C. water level			D. water temperature
61. What device is used to lock the door in the washing machine?
A. a heat-sensitive pellet	B. a mechanical lock		C. a switch	D. key 
62. What provides feedback to the control unit about the door position in the washing machine?
A. a heat-sensitive pellet	B. a mechanical lock		C. a switch	D. key 
63. The machine will not start any program unless the __________ is fully closed and locked. 
A. door		B. clock		C. lock			D. motor
64. When the door is closed, it completes an electrical ________which heats up a heat-sensitive pellet. 
A. electricity		B. cycle		C. circuit		D. electronics
65. __________ expands as it gets hot, pushing a mechanical lock into place and closing a switch. 
A. A heat-sensitive pellet	B. A mechanical lock		C. A switch	D. A key 
66. The ________ signals the control unit that the door is closed and locked. Only when it has received this signal will the control unit start the wash program.
A. heat-sensitive pellet	B.  mechanical lock		C.  switch	D. key 

67. When a wash program first starts it has to open the _______which allow the water in. there are usually two of the _________, one for hot water and for cold. 
A. valve		B. valves		C. pump		D. pumps
68. Each _______ must be controlled separately depending on the water temperature needed for that program. The _______ are solenoid operated, i.e. they are opened and closed electrically.
A. valve/ valve	B. valves/ valve	C. valve/valves	D. valves/valves
69. The rising water level is checked by the water level sensor. This is a_________. The pressure of the air in the plastic tube rises as it is compressed by the rising water. 
A. pressure sensor	B. control		C. air pressure		D. sensor
70. The pressure sensor keeps the control unit informed as to the pressure reached and the control unit uses the information to decide when to close the water________.
A. outlet valves	B. inlet valves		C. inner		D. outer 
71. The____________, a type of thermometer which fits inside the washer drum, measures the water temperature and signals it to the control unit. 
A. water level		B. water sensor	C. temperature sensor		D. pressure sensor
72. The control unit compares it with the temperature needed for the program being used. If the water temperature is__________, the control unit will switch on the heater. 
A. low			B. too low		C. high				D. too high
73. The ___________continues to check the temperature and keep the control unit informed. Once the correct temperature is reached, the control unit switches off the heater and moves on to the next stage of the program.
A. temperature sensor	B. pressure sensor	C. water sensor		D. water level sensor
74. The control unit includes a _________which tells it how long each stage of a program should last. The times may be different for each program. 
A. clock		B. watch		C. memory			D. memories
75. The electronic __________ built into the control unit keeps the memory of the control unit informed so that each stage of each program is timed correctly.
A. clock		B. watch		C. memory			D. memories
76. During the washing and spinning cycles of the program, the _________ has to spin at various speeds. 
A. heater		B. motor		C. fan				D. drum
77. Most machines use three different________: 53 rpm for washing; 83 rpm for distributing the load before spinning; 100 rpm for spinning.
A. speed		B. speeds		C. speedy			D. speech
78.  The control unit signals the motor to produce these speeds. The motor starts up slowly, then gradually increases speed. The_____________, keeps the control unit informed as to the speed that has been reached. The control unit uses the information to control the power to the motor and so controls the speeds of the drum at all times.
A. speed sensor	B.  tachogenerator	C. thermostat			D. A and B are correct.
79. Unless the ignition is switched on, a car cannot ________.
A. start			B. stare		C. started			D. stared
80. Unless the pilot light is on, gas central heating will not_________.
A. worked		B. to work		C. to worked			D. work
81. Unless the diverter valves is switched to central heating, the radiators will not _______.
A. heated 		B. heat up		C. get warm			D. B and C are correct.
82. Unless there is current flowing in the primary coil of a transformer, there will be no current in the _________coil.
A. second		B. origin		C. direct			D. secondary
83. Unless there is __________in the cylinders, a petrol engine will not start.
A. air			B. fuel			C. flow			D. water
84. Unless the doors are __________, a lift will not operate.
A. close		B. shut			C. open			D. connect
85. Unless mild steel is painted, it will __________.
A. corrosion		B. light		C. rust				D. new
86. Unless electrical equipment is earthed, it may be __________.
A. danger		B. safety		C. safe				D. unsafe
87. ___________: is a tube with a very small diameter bore.
A. loop		B. Closed loop		C. Capillary tube		D. compressor
88. __________: a system where part of the output of a system is feedback into the input to modify the output. 
A. loop		B. Closed loop		C. Capillary tube		D. compressor
89. ___________: air at higher than atmospheric pressure; used to power pneumatic devices such as drills.
A. Compressed air	B. Compressor	C. Compression		D. Compress
90. ____________: the effect of forces which act to squash a structure. 
A. Compressed air	B. Compressor	C. Compression		D. Compress
91. __________: a unit where vapour is converted back into a liquid. 
A. Condense		B. Condensing		C. Condensed 			D. Condenser
92. __________: a valve used in central heating to redirect the flow of hot water from radiators to water heating and vice versa.
A. Diverter valve	B. pump		C. cylinder			D. inlet valve
93. ___________: a unit in which a liquid is converted into a vapour.
A. Compressor	B. Condenser		C. Evaporator			D. capillary 
94. __________: a signal responding to the output of a system which is returned to the input to modify the output.
A. Feedback		B. Feed		C. Backwards			D. Receiver 
95. _________: a magnet for producing and maintaining the magnetic field in a generator or electric motor. 
A. Feedback		B. Valve		C. Field magnet		D. magnet
96. ___________: the part of a boiler where the water is heated.
A. Heat exchanger	B. Heat-resistant	C. Pilot light			D. Refrigerant
97. __________: describes a material which will withstand exposure to high temperature.
A. Heat exchanger	B. Heat-resistant	C. Pilot light			D. Refrigerant
98. __________: a small flame used to ignite the main burners in a gas-fired heating boiler.
A. Heat exchanger	B. Heat-resistant	C. Pilot light			D. Refrigerant
99. __________: a substance which changes easily from a liquid to a gas and which can be used in refrigeration to remove heat energy and transfer it to the surroundings.
A. Heat exchanger	B. Heat-resistant	C. Pilot light			D. Refrigerant
100. _________: a control device which operates at a pre-set temperature.
A. Turbine		B. Vapour		C. Thermostat			D. Exchanger
101. __________: a machine which produces power when steam, gas or water is passed over the blades attached to the rotating drive output shaft.
A. Turbine		B. Vapour		C. Thermostat			D. Exchanger
102. _____________: a gas that can be liquided by increasing its pressure.
A. Turbine		B. Vapour		C. Thermostat			D. Exchanger
103. __________is the branch of science dealing with the mechanical action of heat. 
A. Thermostat	B. Thermometer	C. Thermodynamic		D. Thermodynamics
104. Thermodynamics – the science that deals with the relations between _______ and other forms of energy.
A. heat		B. hot			C. cold				D. cool
105. The first law of thermodynamics is that ________can neither be created nor destroyed, but can be converted from one type to another.
A. water		B. fuel			C. energy			D. substance
106. The second law of thermodynamics is that heat always travels from a ______ object to a _______ one.
A. warm/ cold	B. warm/ colder	C. warmer/ hot		D. warm/ hot
107. Heat can travel in any of three ways: __________, conduction, or convection.
A. radio wave	B. radio		C. radiation			D. radiator
108. ___________ is the transfer of heat by waves similar to light waves or radio waves.
A. Radio wave	B. Radio		C. Radiation			D. Radiator
109. ____________is the flow of heat through a substance. Actual physical contact is required for heat transfer to take place between two bodies by this means.
A. Radiation		B. Conduction		C. Convection			D. Refrigeration
110. ____________ is the flow of heat by means of a fluid medium, either gas or liquid, normally air or water.
A. Radiation		B. Conduction		C. Convection			D. Refrigeration
111. In the United States, they normally measure __________in degrees Fahrenheit.
A. temperature	B. water		C. air				D. liquid
112. Air may be heated by a furnace.
113. The sun's energy is transferred to the Earth by radiation.
114. Radiation transfers the sun’s energy to the Earth.
115. The relation between Fahrenheit and Centigrade scales can always be established by the following formulas.
116. Ice was harvested in the winter to be used in the summer.
