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1. ……… engineering deals with making bridges, roads, airports, etc.

A/ Mechanical

B/ Civil

C/ Electrical


D/ Ventilating

2. …….. engineering is about the generation and distribution of electricity and its many applications. 
A/ Mechanical

B/ Civil

C/ Electrical


D/ Ventilating

3. …….….. engineering includes marine, automobile, aeronautical, heating and ventilating, and others. 

A/ Mechanical

B/ Civil

C/ Electrical


D/ Electronic
4. Mining and medical engineering ………… partly ……  mechanical and partly to electrical.

A/ belong/ to


B/ belong / of

C/ belongs/ to 

D/ belongs/ of

5. ….…..: Mechanical engineers design, develop, and make the machines and the processing equipment for harvesting, preparing and preserving the foods and drinks that fill the supermarkets.

A/ Civil


B/ Transport

C/ Medical engineering
D/ Food processing

6 ……..: Electrical engineers provide all the services we need in our homes and places of work, including lighting, heating, ventilation, air-conditioning, refrigeration, and lifts.
A/ Energy and power 



B/ Building services
           
   
C/ Medical engineering



D/ Food processing

7. I work in a ……. I’m responsible for turbine maintenance.

A/ food processing




B/ energy and power              
C/ power station




D/ building services
8 I design ……… They give doctors far more information than X-rays and there’s no risk to the patients.

A/ pictures





B/ photo machines

C/ body scanners




D/ X-ray machines

9/ I’m working with the architects of a new hospital. Getting the …….. right is important. I have to make sure that the working environment will be comfortable for the patients and staff.
A/ generation





B/ refrigeration

C/ lighting





D/ heating and ventilation

10/ Water freezes at ……….and O0C, and water boils at sea level at……... and 1000 C.
A/ 30 0 F/ 200 0 F  




B/ 310 F/ 2100 F

C/ 320 F./ 2120 F  




D/ / 320 F./ 2210 F

11/ Refrigeration preserves food by ........... its temperature.
A/ low



B/ lower

C/ lowering

D/ lows

12/ Pilot light – to………… the boiler.

A/ ignite


B/ start to burn
C/ burn


D/  A and B are correct.



13/ ……… the system is switched on, cold water passes through a heat exchanger in the boiler.

A/ When


B/ As


C/ After

D/on

14/ ..……. the water is pumped to a diverter valve, it goes to the hot water cylinder or the radiators.
A/ When


B/ As


C/ After

D/until

15/ Most gas central heating ………. on the ‘wet’ system of heat transfer between water flowing through pipes.
A/ work


B/ works

C/ working

D/ worked

16/ In conventional boilers, water ………. by gas burners.

A/ heats


B/ is heat

C/ is hot

D/ is heated

17/ Air ……….necessary for complete combustion and ……. supplied to the burners either from inside the house, or directly from outside through a balanced flue.

A/ is/ are


B. are/is

C/ is/ is

D/ are / are
18/ The heat exchanger is made of tubes of cast iron or copper, which ………. corrosion.

A/ resist


B/ resists

C/ resisting

D/ resisted

19/ When this gas is cooled, it …….. back into a liquid.

A/ changes


B/ changing

C/ changed

D/ to change
20/ To keep the refrigerator at a constant low temperature, heat must be transferred from the inside of the cabinet to the outside. A(An) ………….is used to do this.

A/ refrigeration

B/ electrolyte

C/ refrigerant

D/ electrode

21/ The refrigerant has a very low …… point: - 29oC.
A/ refrigerating

B/ heating

C/ cooling

D/ boiling

22/ The refrigeration process begins in the ………..

A/ compressor

B/ condenser

C/ evaporator


D/ refrigerator
23/ Liquid leaving the condenser has to flow down a very narrow tube to prevent liquid from leaving the condenser too quickly, and keeps it at a ……………….

A/ low pressure

B/ high pressure
C/ low pre-set

D/ high pre-set

24/ If a gas is cooled, it changes to ……………
A/ a liquid 


B/ a solid

C/ a gas

D/ a vapour

25/ If a gas ………….., it heats up.

A/ compresses

B/ compressed
C/ is compressed
 D/ will be compressed

26/ If a current passes through a wire,………
A/ it extends in proportion to the force.


B/ there is an equal and opposite reaction.

C/ it sets up a magnetic field around the wire. 

D/ a current is induced in the wire.

27/ If pressure is applied to the surface of an enclosed fluid, …..
A/ it extends in proportion to the force.     

B/ it is transmitted equally throughout the fluid.

C/ it sets up a magnetic field around the wire. 

D/ a current is induced in the wire.

28/ In a refrigeration process, the liquid turns to vapour in the …..
A/ condenser


B/ evaporator


C/ heat exchanger
              D/ capillary tube

29/ The warm gas passes through the condenser, where it……
A/ undergoes changes in pressure and temperature.

B/ the high pressure is maintained.

C/ heats the surroundings and cools down.


D/ expands and cools.






30/ In construction, a complete system of heating, ventilation, and air conditioning is referred to as …….
A/ “HEAT”


B/ “ PUMP” 


C/ “ HVAC” 


D/ “ TEMP”
31/ In the washing machine, the motor rotates the ………
A/ drum


B/ machine


C/ motor


D/ heater

32/ In the washing machine, the solenoid valves control the flow of water ………. the machine.
A/ to



B/ into



C/ out 



D/ out of

33/ In the washing machine, the ……………senses when the drum is full of water and reports it to the control unit.
A/ door lock and sensor
B/ temperature sensor
C/  pressure sensor

D/ fan

34/ In the washing machine, the ………..measures the water temperature and reports it to the control unit.

A/ door lock and sensor
B/ temperature sensor
C/  pressure sensor 

D/ fan
35/ The washing machine will not start any program……… the door ………… fully closed and locked.
A/ unless/ is


B/ if / is

C/ if / is not

D/ A and C are correct.

36/ The heat-sensitive pellet expands as it gets hot, pushing a mechanical lock into place and closing a…
A/ switch


B/ place

C/ unit


D/ position

37/ What device is used to lock the door?

A/ a heat-sensitive pellet
B/ a signal 

C/ a switch

D/ a heatsink
38/ When a wash program first starts it has to………the valves which allow the water in.

A/ opened


B/ to open

C/ opening

D/ open

39/ The rising water level is checked by the…………
A/ level water sensor


B/ sensor water level



C/ water level sensor


D/ water sensor level

40/ What provides feedback to the control unit about the water level?

A/ Solenoid operated valves

B/ Pressure sensor

C/ control unit



D/ Plastic tubes

41/ What provides feedback to the control unit about the water temperature?

A/ Temperature



B/ Temperature sensor

C/ Heater




D/ Thermometer

42/ Most washing machines use ……….. different speeds.

A/ 2


B/ 3


C/4



D/ 5
43/ What device is use to check the drum speeds?

A/ speeds

B/ speed sensor
C/ machine


D/ motor

44/ …………. a wash programme first starts, it opens the valves to allow the water in.

A/ When

B/ As


C/ After


D/ Until

45/ This continues…………the switch contacts are separated.

A/ when

B/ as


C/ after


D/ until
46/ If  the refrigerant R12 is at  -29oC, it  will …………
A/ boil

B/ cools down
C/ heats up


D/ freezes

47/ _________ : a substance which changes easily from a liquid to a gas and which can be used in refrigeration to remove heat energy and transfer it to the surroundings.
A/ refrigerate

B/ refrigeration
C/ refrigerant


D/ refrigerating

48/ __________: a unit in which a liquid is converted into a vapour.

A/ compressor
B. condenser

C. tube


D/ evaporator 
49/ ___________: a device for controlling something from a distance.

A/ thermostat

B. remote control
C. pilot light


D. exchanger

50/ ____________: a small flame used to ignite the main burners in a gas-fired heating boiler.
A/ thermostat

B. remote control
C. pilot light


D. exchanger

_______Hết_______
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