Technical  Data :

	Product  Name : 
	High Precision Mini CNC Milling Machine  

	Product  Item : 
	MM-VM300 

	Control  System : 
	PC-based MACH3 CNC Control System 

	Working  Area 

	Table dimensions : 
	600 X 190 mm

	Table Load capacity : 
	150 KGS 

	Number of T-slots : 
	3 pieces 

	T-slots, width : 
	12 mm 

	T-slots, spacing : 
	49 mm 

	Spindle nose-to-table distance : 
	130—350 mm 

	Throat : 
	235 mm 

	Travels 

	Travel X-Axis : 
	300 mm

	Travel Y-Axis :
	180 mm 

	Travel Z-Axis : 
	290 mm 

	Headstock 

	Spindle  Speed :
	100-6000 RPM 

	Spindle Taper :
	MT3 / BT30

	Max. Moving Speed : 
	8000 mm /min 

	The Max. Feeding Speed : 
	4000 mm /min 

	Position Accuracy :
	±0.02 mm 

	Repeatability Accuracy : 
	±0.01 mm  

	Driving  Capacity 

	Main Motor : 
	1100W / 1500W Powerful Motor 

	X-Axis Motor : 
	4 NM 

	Y-Axis Motor : 
	4 NM 

	Z-Axis Motor : 
	6 NM 

	Max Spindle Motor Torque : 
	5.5 NM 

	Coolant Pump Motor: 
	400W 

	Coolant Tank Capacity : 
	29 Liter 

	Connecting Voltage : 
	Single Phase 240V or Three Phase 400V 

	Measures and Weights 

	Total Driving Motor : 
	4000W 

	Gross  Weight : 
	450 KGS              

	Packing Size : 
	1150 X 1100 X 2000 mm 

	Standard Accessory : 
	MACH3 CNC Control System, Lubrication Equipment
Coolant Pump, Oil Tray, Tools and Tool Box 
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