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Choose the correct answer: 
1. The classic DC motor has a rotating armature in the form of an electromagnet with … poles 
	A. 2
	B. 3
	C. 4
	D. 5


2. …….is a solid-state semiconductor device with four layers of alternating N and P-type material.
	A. Thyristor
	B. Transistor
	C. Triac
	D. Resistor


3.  The speed of the DC motor is proportional to ……...
	A. the current
	B. the voltage
	C. flux
	D. frequency


4. The torque of the DC motor is proportional to……...
	A. flux 
	B. the voltage
	C. the current
	D. frequency


5. The commutator is made up of ………..segments,
	A. gold
	B. steel
	C. silver
	D. copper


[bookmark: _GoBack]6. Rotor refers to the rotating part of a machine such as………
	A. a motor
	B. generator
	C. pump
	D. All are correct


7. What is the resistance of a circuit that takes a current of .5A when the voltage to the circuit is 40V?
	A. 80 ohm
	B. 80 kilo ohm
	C. 8 kilo ohm
	D. 0,8 ohm


8. How many volts are there in 2.7 kV?
	A. 27V
	B. 270V
	C. 2700V
	D. 27000V


9. How much power does a circuit taking .25 A from 12 V supply use:
	A. 3W
	B. 30W
	C. 300W
	D. 3000W


10. What is the current in 0.22 kV, 40 W lamp?
	A. 180A
	B. 180mA
	C. 18A
	D. 18mA


The transformer is one of the …(11)…of electrical devices. Its basic design, materials, and principles …(12)….little over the last one hundred years, yet transformer designs and materials continue to…(13)…. …(14)….are essential in …(15)…..voltage power transmission providing an economical means of transmitting power over …(16)…..distances. The simplicity, reliability, and …(17)…..of conversion of …(18)……by transformers was the principal factor in the selection of …(19)…. current power transmission in the "War of Currents" in the …(20)…..1880's
	11. A. simplest
	B. complex
	C. simple
	D. compound

	12. A. changed
	B. has changed
	C. have changed
	D. None is correct

	13. A. improved
	B. be improved
	C. developed
	D. be developed

	14. A. Transformers
	B. Inverters
	C. Contactors
	D. Encoders

	15. A. high
	B. low
	C. small
	D. big

	16. A. small
	B. large
	C. high
	D. low

	17. A. economical
	B. economy
	C. economic
	D. All are correct

	18. A. currents
	B. powers
	C. voltages
	D. All are correct

	19. A. alternating
	B. direct
	C. directing
	D. alternate

	20. A. early
	B. first
	C. mid
	D. late


21. The movement of free electrons towards the positive end.
	A. Electric current
	B. Electric motor
	C. Direct current
	D. Alternating current


22. A current which flows first in one direction, then in the other.
	A. Electric current
	B. Electric motor
	C. Direct current
	D. Alternating current


23. A current which flows in one direction only.
	A. Electric current
	B. Electric motor
	C. Direct current
	D. Alternating current


24. A device which converts electrical energy into mechanical energy.
	A. Electric current
	B. Electric motor
	C. Direct current
	D. Alternating current


25. A device which changes chemical energy into electrical energy.
	A. Generator
	B. Battery
	C. Resistor
	D. Ammeter


26. An instrument which measures current.
	A. Generator
	B. Battery
	C. Resistor
	D. Ammeter


27. A device which is used to add resistance to a circuit
	A. Generator
	B. Battery
	C. Resistor
	D. Ammeter


28. A device which converts mechanical energy into electrical energy.
	A. Generator
	B. Battery
	C. Resistor
	D. Ammeter


29. Materials which provide an easy path for an electric current.
	A. Conductors
	B. Insulators
	C. Semiconductors
	D. All are correct


30. Materials which do not easily release electrons.
	A. Conductors
	B. Insulators
	C. Semiconductors
	D. All are correct


31. A two-hundred-and-twenty-kilohm resistor.
	A. R1
	B. P1
	C. L1
	D. C2


32. A hundred-picofarad (puff) capacitor.
	A. R1
	B. P1
	C. L1
	D. C2


33. When A is high and B is low, the output is low.
	A. AND
	B. NAND
	C. NOT
	D. All are correct


34. When the input is low, the output is high.
	A. AND
	B. OR
	C. NOT
	D. NAND


35. When A and B are high, the output is high
	A. NAND
	B. OR
	C. NOT
	D. All are correct


36. When A and B are high, the output is low
	A. AND
	B. OR
	C. NOT
	D. NAND


37. When the input is high, the output is low
	A. AND
	B. OR
	C. NOT
	D. NAND


38. When A and B are low, the output is high
	A. AND
	B. OR
	C. NOT
	D. NAND


39. When A is low and B is high, the output is low.
	A. AND
	B. NAND
	C. NOT
	D. OR


40. When A is low and B is high, the output is high.
	A. AND
	B. NAND
	C. NOT
	D. All are correct


41. Rated current up to 100A.
	A. MCB
	B. MCCB
	C. ACB
	D. VCB


42. Rated current up to 1000A.
	A. MCB
	B. MCCB
	C. ACB
	D. VCB


43. Rated current up to 10000A.
	A. MCB
	B. MCCB
	C. ACB
	D. VCB


44. Rated current up to 3000A.
	A. MCB
	B. MCCB
	C. ACB
	D. VCB


45. It's used to change AC voltages from small to large or from large to small.
	A. a logic probe
	B. a motion sensor
	C. a multi meter
	D. a transformer


46. It's used for measuring very small currents.
	A. a logic probe
	B. a motion sensor
	C. a multi meter
	D. a transformer


47. It's used to check the logic levels in the pins of ICs.
	A. a logic probe
	B. a motion sensor
	C. a multi meter
	D. a transformer


48. It's used as part of a burglar alarm to detect movement.
	A. a logic probe
	B. a motion sensor
	C. a multi meter
	D. a transformer


49. It's used for the transmission of RF signals.
	A. a circuit breaker.
	B. a transmitter aerial.
	C. a metal detector
	D. a mixer.


50. …………is a device used to encode a signal
	A. A contactor
	B. An inverter
	C. A sensor
	D. An encoder
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