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Choose the correct answer:
The transformer is one of the …(1)…of electrical devices. Its basic design, materials, and principles …(2)….little over the last one hundred years, yet transformer designs and materials continue to…(3)…. …(4)….are essential in …(5)…..voltage power transmission providing an economical means of transmitting power over …(6)…..distances. The simplicity, reliability, and …(7)…..of conversion of …(8)……by transformers was the principal factor in the selection of …(9)…. current power transmission in the "War of Currents" in the …(10)…..1880's
	1. A. simplest
	B. complex
	C. simple
	D. compound

	2. A. changed
	B. has changed
	C. have changed
	D. None is correct

	3. A. improved
	B. be improved
	C. developed
	D. be developed

	4. A. Transformers
	B. Inverters
	C. Contactors
	D. Encoders

	5. A. high
	B. low
	C. small
	D. big

	6. A. small
	B. large
	C. high
	D. low

	7. A. economical
	B. economy
	C. economic
	D. All are correct

	8. A. currents
	B. powers
	C. voltages
	D. All are correct

	9.  A. alternating
	B. direct
	C. directing
	D. alternate

	10. A. early
	B. first
	C. mid
	D. late


11. ……….detect current imbalance
	A. RCD
	B. ELCB
	C. CB
	D. RCBO


12. ……….detect earth current
	A. RCD
	B. ELCB
	C. CB
	D. RCBO


13. ……….overload or short circuit protection. 
	A. RCD
	B. ELCB
	C. CB
	D. RCBO


14.  ……….fault and over-current protection.
	[bookmark: _GoBack]A. RCD
	B. ELCB
	C. CB
	D. RCBO


15. …………is an electrical device used for controlling power flow.
	A. A contactor
	B. An inverter
	C. A sensor
	D. An encoder


16. …………is a device used to encode a signal
	A. A contactor
	B. An inverter
	C. A sensor
	D. An encoder


17. …………is a device that detects and responds to some type of input from the physical environment
	A. A contactor
	B. An inverter
	C. A sensor
	D. An encoder


18. ………..is an electric device that changes direct current (DC) to alternating current (AC)
	A. An inverter
	B. A contactor
	C. A sensor
	D. An encoder


19. ………..is an electrical switch that periodically reverses the current in an electric motor or electrical generator
	A. Inverter
	B. Commutator
	C. Contactor
	D. None is correct


20 ………..is one of the two principal components of an electro-mechanical machine-a motor or generator
	A. Commutator
	B.  Contactor
	C. Armature
	D. all are correct


21. ………..can be thought of informally as "rotational force".
	A. Torque
	B.  Moment
	C. Armature
	D. A and B are correct


22. Alternating current is abbreviated to………
	A. DC
	B. AC
	C. AD
	D. None is correct


23. Direct current is abbreviated to………….
	A. AC
	B. CD
	C. DC
	D. None is correct


24. DC generator contains ratings as: ………
	A. voltage, current
	B. power, speed.
	C. power, current.
	D. both of A and B


25. The classic DC motor has a rotating armature in the form of an electromagnet with … poles 
	A. 3
	B. 2
	C. 4
	D. None is correct


26. Rotor refers to the rotating part of a machine such as………
	A. a motor
	B. generator
	C. pump
	D. all are correct


27. ROM is the abbreviation of:
	A. Red-Only Memory
	B. Read-On Memory
	C. Read-Only Memory
	D. Red-On Memory


28. ……....using standard electronic symbols to show how electronic components are connected together. 
	A. Component
	B. Circuit diagram
	C. Collector
	D. Block diagram


29. RAM is the abbreviation of:
	A. Random-Access Memory
	B. Radio-access Memory
	C. Read-access Memory
	D. Red-access Memory


30. CPU is the abbreviation of:
	A. Centre Process Unit
	B. Central Processing Unit
	C. Central Program Unit
	D. Center Processing Unit


31. It was not until 1958 that microelectronics began ……..the development of ICs (integrated circuits) on silicon chips
	A. with
	B. to
	C. at
	D. for


32. The ……. is used to transfer data between all the units
	A. data bus
	B. CPU
	C. control bus
	D. address bus


33. The ……..is used to send control signals from the CPU to the other units
	A. address bus
	B. data bus
	C. CPU
	D. control bus


34. The …….. is used to send signals from the CPU which indicate the memory and I/O locations to be used
	A. address bus
	B. data bus
	C. CPU
	D. control bus


35. The CPU is a microprocessor. “ micro” means:
	A. big
	B. large
	C. small
	D. great


36. “  Semi” in the word…“ Semiconductor”  is a….…which means 'half’. 
	A. suffix 
	B. prefix
	C. prefixes
	D. all are correct 


37.  It's used for protecting circuits from a surge in voltage.
	A. a surge fuse
	B. a fuse
	C. a circuit breaker
	D. all are correct


38. It's used for measuring very small currents.
	A. a microammeter
	B. a milliammeter
	C. a multimeter
	D. all are correct


39. The operation of  MCB is ………..
	A. electronic
	B. thermal
	C. thermal-magnetic
	D. B and C are correct


40. Air circuit breaker rates current up to ………
	A. 10,000 mA
	B. 10,000 A
	C. 1000 A
	D. 3000 A


41. ……………..is a loop of wire, often wrapped around a metallic core, which produces a magnetic field when an electrical current is passed through it.
	A. Solenoid
	B. Contacts
	C. Actuator level
	D. Calibration screw


42. ……………..used to manually trip and reset the circuit breaker. Also indicates the status of the circuit breaker (On or Off/tripped).
	A. Contacts
	B. Solenoid
	C. Actuator level
	D. Calibration screw


43. ……………forces the contacts together or apart.
	A. Actuator mechanism
	B. Contacts
	C. Solenoid
	D. Actuator level


44. ……….allow current to flow when touching and break the flow of current when moved apart
	A. Calibration screw
	B. Actuator level
	C. Solenoid
	D. Contacts


45. ………..allows the manufacturer to precisely adjust the trip current of the device after assembly. 
	A. Actuator level
	B. Calibration screw
	C. Contacts
	D. Solenoid


46. ………..is used to convert a temperature change into mechanical displacement.
	A. Bimetallic strip
	B. Solenoid
	C. Contact
	D. Actuator level


47. What is the resistance of a circuit that takes a current of .5 A when the voltage to the circuit is 40V?.
	A. 80 ohm
	B. 80 kilo ohm
	C. 8 kilo ohm
	D. 0,8 ohm


48. How many volts are there in 2.7 kV?
	A. 27V
	B. 270V
	C. 2700V
	D. None is correct


49. How much power does a circuit taking .25 A from a 12 V supply use:
	A. 3W
	B. 30W
	C. 3KW
	D. all are correct


50. What is the current in a 0.22 kV, 40 W lamp?
	A. 1,8A
	B. 180mA
	C. 18A
	D. 18mA
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