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Choose the correct answer:
1. …... ...are burned in large furnaces to heat water to make steam that in turn pushes on the blades of a turbine.
	A. Coal
	B. Petroleum(oil)
	C. Natural gas
	D. All are correct


2……. comes from heat energy buried beneath the surface of the earth.
	A. Geothermal power
	B. Solar power
	C. Nuclear power
	D. Wind power  


3.......... is a method in which steam is produced by heating water through a process called nuclear fission.
	A. Solar power
	B. Geothermal power
	C. Nuclear power
	D. Wind power  


 4.......... is derived from the energy of the sun
	A. Nuclear power 
	B. Geothermal power
	C. Solar power
	D. Wind power  


5............., electricity generation, is a process in which flowing water is used to spin a turbine connected to a generator
	A. Nuclear power 
	B. Hydro power
	C. Solar power
	D. Geothermal power


6..............is derived from the conversion of the energy contained in wind into electricity.
	A. Wind power  
	B. Geothermal power
	C. Solar power
	D. Nuclear power


7. Electronics began at the startof the twentieth century with the invention of …….
	A. The transistor
	B. Vacuum tube
	C. ICs
	D. Robots


8. A wide variety of electronic devices such as hi-fi units and portable radios became common in the homeby the invention of…… in 1947
	A. The transistor
	B. ICs
	C. Vacuum tube
	D. Robots


9.  IC  is the abbreviation of:
	A. Input Circuit
	B. Integrated Circuit
	C. Information Center
	D. Identity Card



The transformer is one of the …(10)…of electrical devices. Its basic design, materials, and principles …(11)….little over the last one hundred years, yet transformer designs and materials continue to…(12)…. …(13)…. are essential in …(14)…..voltage power transmission providing an economical means of transmitting power over …(15)…..distances. The simplicity, reliability, and …(16)…..of conversion of …(17)……by transformers was the principal factor in the selection of …(18)…. current power transmission in the "War of Currents" in the …(19)…..1880's
	10. A. simplest
	B. complex
	C. simple
	D. compound

	11. A. changed
	B. has changed
	C. have changed
	D.None is correct

	12. A. improved
	B. be improved
	C. develop
	D. be developed

	13. A. Transformers
	B. Inverters
	C. Contactors
	D. Encoders

	14. A. high
	B. low
	C. small
	D. big

	15. A. small
	B. large
	C. high
	D. low

	16. A. economical
	B. economy
	C. economic
	D. All are correct

	17. A. currents
	B. powers
	C. voltages
	D. All are correct

	18.  A. alternating
	B. direct
	C. directing
	D. alternate

	19. A. early
	B. first
	C. mid
	D. late


20. The radioconsists ofa tuner, a detector, and an AF amplifier. “ consists of” means:
	A. comprise
	B. is composed of
	C. composes
	D. none is correct


21. The tuneris connected tothe detector.   “is connected to  ” means:
	A. is linked to
	B. are linked to
	C. is linked 
	D. are linked 


[bookmark: _GoBack]22. A tuner, a detector, and an AF amplifier ……..theradio.
	A. comprises
	B. to comprise
	C. comprising
	D. comprise


23. Do you have access to a computer ?
	A. yes, I don’t
	B. yes, I do
	C. No, I do
	D. None is correct


24. We can access to a computer:
	A. at home
	B. at work
	C. at college
	D. all are correct


25. We can use computer for:
	A. learning English
	B. entertainment
	C. playing games
	D. all are correct


26. The ……. is used to transfer data between all the units
	A. data bus
	B. CPU
	C. control bus
	D. address bus


27. The ……..is used to send control signals from the CPU to the other units
	A. address bus
	B. data bus
	C. CPU
	D. control bus


28. The …….. is used to send signals from the CPU which indicate the memory and I/O locations to be used
	A. address bus
	B. data bus
	C. CPU
	D. control bus


29. The CPU is a microprocessor. “ micro” means:
	A. big
	B. large
	C. small
	D. great


30. “  Semi” in the word…“ Semiconductor”  is a….…which means 'half’. 
	A. suffix 
	B. prefix
	C. prefixes
	D. all are correct 


31.  It's used for protecting circuits from a surge in voltage.
	A. a surge fuse
	B. a fuse
	C. a circuit breaker
	D. all are correct


32. It's used for measuring very small currents.
	A. a microammeter
	B. a milliammeter
	C. a multimeter
	D. all are correct


33. The operation of MCB is ………..
	A. electronic
	B. thermal
	C. thermal-magnetic
	D. B and C are correct


34. Air circuit breaker rates current up to ………
	A. 10,000 mA
	B. 10,000 A
	C. 1000 A
	D. 3000 A


35. ……………..is a loop of wire, often wrapped around a metallic core, which produces a magnetic field when an electrical current is passed through it.
	A. Solenoid
	B. Contacts
	C. Actuatorlevel
	D. Calibration screw


36. ……………..used to manually trip and reset the circuit breaker. Also indicates the status of the circuit breaker (On or Off/tripped).
	A. Contacts
	B. Solenoids
	C. Actuatorlevel
	D. Calibration screw


37. ……………forces the contacts together or apart.
	A. Actuator mechanism
	B. Contacts
	C. Solenoids
	D. Actuator level


38. ……….allow current to flow when touching and break the flow of current when moved apart
	A. Calibration screw
	B. Actuator level
	C. Solenoids
	D. Contacts


39. ………..allows the manufacturer to precisely adjust the trip current of the device after assembly. 
	A. Actuator level
	B. Calibration screw
	C. Contacts
	D. Solenoids


40. ………..is used to convert a temperature change into mechanical displacement.
	A. Bimetallic strip
	B. Solenoids
	C. Contacts
	D. Actuator level


41. ……….detect current imbalance
	A. RCD
	B. ELCB
	C. CB
	D. RCBO


42. ……….detect earth current
	A. RCD
	B. ELCB
	C. CB
	D. RCBO


43. ……….overload or short circuit protection. 
	A. RCD
	B. ELCB
	C. CB
	D. RCBO


44.  ……….fault and over-current protection.
	A. RCD
	B. ELCB
	C. CB
	D. RCBO


45. …………is an electrical device used for controlling power flow.
	A. A contactor
	B. An inverter
	C. A sensor
	D. An encoder


46. …………is a device used to encode a signal
	A. A contactor
	B. A inverter
	C. A sensor
	D. An encoder


47. …………is a device that detects and responds to some type of input from the physical environment
	A. A contactor
	B. An inverter
	C. A sensor
	D. An encoder


48. ………..is an electric device that changes direct current (DC) to alternating current (AC)
	A. Aninverter
	B. A contactor
	C. A sensor
	D. An encoder


49. ………..is an electrical switch that periodically reverses the current in an electric motor or electrical generator
	A. Inverter
	B. .Commutator
	C. Contactor
	D. None is correct


50 ………..is one of the two principal components of an electro-mechanical machine-a motor or generator
	A. Commutator
	B. A Contactor
	C. Armature
	D. all are correct


51. ………..can be thought of informally as "rotational force".
	A. Torque
	B. A moment
	C. Armature
	D. A and B are correct


52. Alternating current is abbreviated to………
	A. DC
	B. AC
	C. AD
	D. None is correct


53. Direct current is abbreviated to………….
	A. AC
	B. CD
	C. DC
	D. None is correct


54. DC generator contains ratings as: ………
	A. voltage, current
	B. power, speed.
	C. power, current.
	D. both of A and B


55. The classic DC motor has a rotating armature in the form of an electromagnet with … poles 
	A. 3
	B. 2
	C. 4
	D. None is correct


56. ….is a solid-state semiconductor device with four layers of alternating N and P-type material.
	 A. Thyristor
	B. Transistor
	C. Triac
	D. all are correct 


57.  The speed of the DC motor is proportional to ……...
	A. the current
	B. the voltage
	C. flux
	D. A and B are correct


58. The torque of the DC motor is proportional to……...
	A. flux 
	B. the voltage
	C. the current
	D. all are correct


59. The commutator is made up of ………..segments,
	A. gold
	B. steel
	C. silver
	D. copper


60. Rotor refers to the rotating part of a machine such as………
	A. a motor
	B. generator
	C. pump
	D. all are correct


61. What is the resistance of a circuit that takes a current of .5 A when the voltage to the circuit is 40V?.
	A. 80 ohm
	B. 80kilo ohm
	C. 8kilo ohm
	D. 0,8ohm


62. How many volts are there in 2.7 kV?
	A. 27V
	B. 270V
	C. 2700V
	D. None is correct


63. How much power does a circuit taking .25 A from a 12 V supply use:
	A. 3W
	B. 30W
	C. 3KW
	D. all are correct


64. What is the current in a 0.22 kV, 40 W lamp?
	A. 1,8A
	B. 180mA
	C. 18A
	D. 18mA


65. It was not a problem. We looked ………his number in the telephone book
	A. up
	B. for
	C. on
	D. in


66. The plane took …… very quickly.
	A. of
	B. on
	C. off
	D. in


67. Anne is leaving ……. London tomorrow morning
	A. on
	B. for
	C. with
	D. in


68. If there was a technical failure, Gagarin might never get ……… to the Earth
	A. of
	B. off
	C. in
	D. back


69. I’m good……… English, but I’m bad………. Mathematics
	A. at/at 
	B. about/at
	C. at/about
	D. in/in


70.  Her parents are very pleased……… her French.
	A. about
	B. on
	C. with
	D. of


71. I’m not interested ……….. politics
	A. in
	B. for
	C. about
	D. with


72. She was sad because he was very rude………. her.
	A. with
	B. off
	C. of
	D. to


73. Thank you. It was very kind……….. you to help me
	A. off
	B. of
	C. for
	D. with


74. Can you send it to me …….. fax?.
	A. with
	B. in
	C. by
	D. for


Microprocessors are now…. (75)… control many household items …(76)…automatic washing-machines, dishwashers, …(77)….heatingsystems, sewing machines, and food processors. Electronic timers …(78)… in digital alarm clocks, water heaters, electric cookers, and microwave ovens.  …(79)….use electronics to …(80)…automatic dialling and answerphone facilities. New entertainment devices …(81)…developed, such as video recorders and CD (compact disc) players.
…(82)…, electronics are likely to become even more common in the home …(83)…multimedia entertainment systems and computer-controlled robots…(84)….
	75. A. use
	B. using
	C. used to
	D. used for

	76. A. like
	B. such as
	C. as
	D. All are correct

	77. A. center
	B. central
	C. centre
	D. All are correct

	78. A. found
	B. is found
	C. are found
	D. none is correct

	79. A. Televisions
	B. Radios
	C. Compurters
	D. Telephones

	80. A. provide
	B. supply
	C. give
	D. have

	81. A. has been
	B. had been
	C. have been
	D. have

	82. A. Today
	B. In the future
	C. In the past
	D. Nowadays

	83.  A. as
	B. like
	C. such as
	D. All are correct

	84. A. developed
	B. have developed
	C. is developed
	D. are developed


85. The output of a gate for all possible inputs?
	A. TTL and CMOS
	B. a pin-out diagram
	C. an inverter
	D. a truth table


86 The arrangement of the gates and the function of each pin on the chip
	A. a pin-out diagram 
	B. TTL and CMOS
	C. an inverter
	D. a truth table


87. What is another name for a NOT gate?
	A. a pin-out diagram 
	B. TTL and CMOS
	C. a truth table
	D. an inverter


88. What are the two common families of logic ICs?
	A. a pin-out diagram 
	B. TTL and CMOS
	C. a truth table
	D. an inverter


89. The number of ICs used in a computer
	A. logic gate
	B. combinational
	C. chip count
	D. scale of integration


90. The circuit breakers are like the fuses.
		A. True
	B.False


91. The operation of MCB is electronic.
		A. True
	B. False


92. The trip current of MCB cannot be adjustable.
		A. True
	B. False


93. Air circuit breaker rates current up to 10,000 mA
		A. True
	B. False


94. Most magnetic motors are stationary.
		A. True
	B. False


95. When a transformer is used to “increase” the voltage on its secondary winding with respect to the primary, it is called a step-up transformer.
		A. True
	B. False


96. Depending upon the design of the machine, not only rotor but also stator	
serve as the armature.
		A. True
	B. False


97. Transformers are not often used to convert between high and low voltages.	
		A. True
	B. False


98. Transformers alone can Convert DC to AC or vice versa. 
		A. True
	B. False


99. Transformers alone can not change the voltage or current of DC.
		A. True
	B. False


100.When it is used to “decrease” the voltage on the secondary winding with respect to the primary it is called a step-down transformer.
		A. True
	B. False
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