ỌC PHẦN : ANH VĂN CHUYÊN NGÀNH

ĐỀ 1

 Fill in the gaps in the following sentences by using multiple choices:
1. …... ...are burned in large furnaces to heat water to make steam that in turn pushes on the blades of a turbine.

	A. Coal
	B. Petroleum(oil)
	C. Natural gas
	D. All are correct


2……. comes from heat energy buried beneath the surface of the earth.

	A. Geothermal power
	B. Solar power
	C. Nuclear power
	D. Wind power  


3.......... is a method in which steam is produced by heating water through a process called nuclear fission.

	A. Solar power
	B. Geothermal power
	C. Nuclear power
	D. Wind power  


 4.......... is derived from the energy of the sun
	A. Nuclear power 
	B. Geothermal power
	C. Solar power
	D. Wind power  


5............., electricity generation, is a process in which flowing water is used to spin a turbine connected to a generator

	A. Nuclear power 
	B. Hydro power
	C. Solar power
	D. Geothermal power


6..............is derived from the conversion of the energy contained in wind into electricity.

	A. Wind power  
	B. Geothermal power
	C. Solar power
	D. Nuclear power


7. Electronics began at the start of the twentieth century with the invention of …….
	A. The transistor
	B. Vacuum tube
	C. ICs
	D. Robots


8. A wide variety of electronic devices such as hi-fi units and portable radios became common in the home by the invention of…… in 1947
	A. The transistor
	B. ICs
	C. Vacuum tube
	D. Robots


9.  IC   the abbreviation of:
	A. Input Circuit
	B. Integrated Circuit
	C. Information Center
	D. Identity Card


10. CD   the abbreviation of:
	A. Compact Disc
	B. Current Directory
	C. Control Data
	D. Center Director


11. ROM   the abbreviation of:

	A. Red-Only Memory
	B. Read-On Memory
	C. Read-Only Memory
	D. Red-On Memory


12. Drawing using standard electronic symbols to show how electronic components are connected together. This statement refer to:
	A. component
	B. circuit diagram
	C. Collector
	D. block diagram


13. RAM   the abbreviation of:
	A. Random-Access Memory
	B. Radio-access Memory
	C. Read-access Memory
	D. Red-access Memory


14. CPU the abbreviation of:

	A. Centre Process Unit
	B. Central Processing Unit
	C. Central Program Unit
	D. Center Processing Unit


15. It was not until 1958 that microelectronics began ……..the development of ICs (integrated circuits) on silicon chips
	A. with
	B. to
	C. at
	D. for


16. Microprocessors are now used ……. control many household itemssuch as automatic washing-machines, dishwashers central heating systems, and food processors.
	A. with
	B. to
	C. at
	D. for


17. Microprocessors are now used ……. control many household itemssuch as automatic washing-machines, dishwashers central heating systems, and food processors.
	A. with
	B. to
	C. at
	D. for


18. The RAM is used …….temporary storage of programs and data
	A. with
	B. to
	C. at
	D. for


19. Electronic devices are made …….common basic units connected together

	A. up off
	B. up to
	C. up of
	D. up for


20. The radio consists of  a tuner, a detector, and an AF amplifier. “ consists of  ” means:
	A. comprise
	B. is composed of
	C.  composes 
	D. none is correct


21. The tuner is connected to the detector.   “  is connected to  ” means:
	A. is linked to
	B. are linked to
	C. is linked 
	D. are linked 


22. A tuner, a detector, and an AF amplifier ……..the radio.
	A. comprises
	B. to comprise
	C. comprising
	D. comprise


23. Do you have access to a computer ?
	A. yes, I don’t
	B. yes, I do
	C. No, I do
	D. None is correct


24. We can access to a computer:
	A. at home
	B. at work
	C. at college
	D. all are correct


25. We can use computer for:
	A. learning English
	B. entertainment
	C. playing games
	D. all are correct


26. The ……. is used to transfer data between all the units
	A. data bus
	B. CPU
	C. control bus
	D. address bus


27. The ……..is used to send control signals from the CPU to the other units
	A. address bus
	B. data bus
	C. CPU
	D. control bus


28. The …….. is used to send signals from the CPU which indicate the memory and I/O locations to be used

	A. address bus
	B. data bus
	C. CPU
	D. control bus


29. The CPU is a microprocessor. “ micro” means:
	A. big
	B. large
	C. small
	D. great


30. “  Semi  ” in the word…“ Semiconductor”  is a….…which means 'half’. 

	A. suffix 
	B. prefix 
	C. raffix 
	D. all are correct 


31.  It's used for protecting circuits from a surge in voltage.

	A. a surge fuse
	B. a fuse
	C. a circuit breaker
	D. all are correct


32. It's used for measuring very small currents.

	A. a microammeter
	B. a milliammeter
	C. a multimeter
	D. all are correct


The output of each gate depends on the combination of its…(33)…. This is known as combinational logic. The …(34)…..for all possible inputs is shown using a truth table. The truth tables show that the …(35)...of an AND gate is only …(36)  ....(i.e. logic level 1) when all its …(37)….are high. The output of a …(38)...gate, however, stays high unless all its inputs are…(39)….. The output of a NOT gate (also known as an inverter) is always the ...(40)... of its input .
	
	
	
	

	33. A. input
	B. outputs
	C. inputs
	D. output

	34. A. input
	B. output
	C. inputs
	D. outputs

	35. A. outputs
	B. input
	C. intputs
	D. output

	36. A. low
	B. high
	C. hight
	D. lower

	37. A. input
	B. inputs
	C. outputs
	D. output

	38. A. NAND
	B. AND
	C. OR
	D. NOT

	39.  A. high
	B. low
	C. hight
	D. lower

	40. A. opposited
	B. reverse
	C. invert
	D. opposite
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